For 1990-2009 cars

### Removal Procedure

1. Lower the door window.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
4. Remove the window run channel weatherstrip:

• | Start at the upper rear corner of the door frame.

• | Pull out the weatherstrip.

### Installation Procedure

1. Install the window weatherstrip:

• | Start at the upper rear corner of the door frame.

• | Insert the weatherstrip into the channel.

2. Install the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
4. Close the door window.