For 1990-2009 cars

### Removal Procedure

Important: Tape above and below the molding in order to prevent damage to the painted surfaces when removing the molding. Replace the front fender center molding after you have removed it. Paint the center molding prior to installation. Refer to Basecoat/Clearcoat Paint Systems in Paint Coatings.

1. Perform the following steps in order to remove the molding:

1.1. | Start at the rear of the molding.

1.2. | Pull the molding away from the fender.

1.3. | Use a plastic tool in order to pry the molding from the fender.

2. Use an oil-free naphtha or use isopropyl alcohol in order to clean the door surfaces.

### Installation Procedure

1. Use a heat gun or use a heat lamp in order to warm the body panel to a minimum temperature of 21°C (70°F).
2. Peel the backing from the molding.
3. Align the molding and the clips with the door holes. Do NOT overlap the molding over the door edge or over the door edge guard.
4. Insert the center molding.
5. Press the center molding firmly.