For 1990-2009 cars

### Removal Procedure

1. Disconnect the wiring harness from the IAT sensor (1).
2. Remove the IAT sensor with the rubber grommet carefully from the air intake duct.

Notice: Excessive force may damage the sensor.

3. Remove the rubber grommet from the IAT sensor.

### Installation Procedure

1. Install the rubber grommet onto the IAT sensor (1). Observe the installation position.
2. Install the IAT sensor with the rubber grommet into the air intake duct.

Notice: Excessive force may damage the sensor.

3. Connect the wiring harness to the IAT sensor.