For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat to back window panel. Refer to Rear Window Trim Panel Replacement .
2. Remove six nuts retaining sunshade to the rear seat to back window panel.
3. Remove sunshade from the rear seat to back window panel.

### Installation Procedure

1. Install the sunshade to rear seat to back window panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the six nuts to secure the sunshade to the rear seat to back window panel.

Tighten
Tighten sunshade nuts fully seated and nut stripped.

3. Install the rear seat to back window panel. Refer to Rear Window Trim Panel Replacement .