For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Release the taillamp cover clips.
3. Remove the taillamp cover.
4. Remove the bulb socket from the taillamp.
5. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket.
2. Install the bulb socket to the taillamp.
3. Install the taillamp cover.
4. Secure the taillamp cover clips.
5. Close the rear compartment lid.