For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C High Pressure Switch | 7 N·m | 62 lb in
A/C Pressure Sensor | 7 N·m | 62 lb in
Blower Motor Housing Screw | 4 N·m | 35 lb in
Center Console Support Brace Nut - Rear | 8 N·m | 71 lb in
Compressor Drain Plug | 20 N·m | 15 lb ft
Compressor Hose Bolt | 33 N·m | 24 lb ft
Compressor Hose Bracket to Air Pipe Bolt | 8 N·m | 71 lb in
Compressor Hose Bracket to Oil Pan Bolt | 8 N·m | 71 lb in
Compressor Mounting Bolt | 40 N·m | 30 lb ft
Compressor Pressure Relief Valve | 9 N·m | 80 lb in
Condenser Tube Block Fitting Bolt | 27 N·m | 20 lb ft
Condenser Tube Fitting Nut | 44 N·m | 33 lb ft
Evaporator Tube Extension Block Fitting Bolt | 20 N·m | 15 lb ft
Evaporator Tube Extension Fitting Nut | 44 N·m | 33 lb ft
Evaporator Tube Screw | 5 N·m | 44 lb in
Heater Core Pipe Retaining Bracket Screw | 5 N·m | 44 lb in
HVAC Module Nut - Passenger Compartment | 4 N·m | 35 lb in
HVAC Module Screw - Engine Compartment | 4 N·m | 35 lb in
IP Support Bracket Bolt | 22 N·m | 16 lb ft
Rear Air Outlet Duct Screw | 4 N·m | 35 lb in
Receiver/Dehydrator Block Fitting Bolt | 15 N·m | 11 lb ft
Receiver/Dehydrator Bracket Bolt | 4 N·m | 35 lb in
Thermal Expansion Valve (TXV) Screw | 8 N·m | 71 lb in