For 1990-2009 cars

### Removal Procedure

1. Disconnect the AIR Cutoff Valve Vacuum Control solenoid wiring harness connector.
2. Disconnect the vacuum hoses observing the proper positions.
3. Remove the solenoid bracket fasteners.
4. Disconnect the solenoid electrical connector.
5. Remove the assembly from the vehicle.
6. Remove the valve from the bracket.

### Installation Procedure

1. Install the valve to the bracket.
2. Install the assembly to the vehicle.
3. Install/tighten the bracket fasteners.
4. Reconnect the vacuum hoses in the correct positions.
5. Reconnect the electrical connector.