For 1990-2009 cars

### Removal Procedure

1. Open the door.
2. Remove the door jamb switch screw.
3. Remove the door jamb switch from the center pillar.
4. Disconnect the jamb switch connectors.

### Installation Procedure

1. Connect the door jamb switch electrical connectors.

Position the door jamb switch to the center pillar.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the door jamb switch screw.

Tighten
Tighten the door jamb switch screw to 6 N·m (53 lb in).

3. Close the door.