For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Pull the release handles which are located at the base of rear seat cushion.
2. Remove the rear seat cushion heating element electrical connectors (1).
3. Remove the rear seat belt from lower seat cushion.
4. Remove the rear seat cushion from vehicle.

### Installation Procedure

1. Install the rear seat cushion to vehicle.
2. Install the rear seat belt to lower seat cushion.
3. Install the rear seat cushion heating element electrical connectors (1).
4. Install the rear seat cushion. Insert the rear seat cushion to inner floor pan. Push downward to lock in place.