For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Remove the backup lamp access cover by pressing the tabs together and pulling the cover from the rear compartment lid.
3. Remove the backup lamp bulb/socket from the backup lamp by pressing the tabs together.
4. Remove the bulb from the bulb/socket.

### Installation Procedure

1. Install the backup lamp bulb to the bulb/socket.
2. Install the backup lamp bulb/socket to the backup lamp, pressing until fully seated.
3. Install the backup lamp access cover.
4. Close the rear compartment.