For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .

Important: The tab is located at the base of the rear seatback outer cushion.

2. Remove the rear seatback outer cushion by bending the tab outward and pushing upward on the rear seatback outer cushion in order to release the tab from the hook.

### Installation Procedure

1. Install the rear seatback outer cushion.
2. Place the rear seatback cushion on the hook and push downward in order to lock the tab in place.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .