For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement in Exterior Trim.
2. Remove the screw located in the upper corner of each headlamp lower trim.
3. Unhook the edge or the headlamp lower trim from the fender.
4. Remove the headlamp lower trim.

### Installation Procedure

1. Hook the headlamp lower trim to the fender to install.
2. Check that the headlamp lower trim is aligned with the fender.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the headlamp lower trim screw.

Tighten
Tighten the headlamp lower trim screw until fully seated. DO NOT strip the headlamp lower trim screw.

4. Install the grille. Refer to Grille Replacement in Exterior Trim.