For 1990-2009 cars

• |
- Vehicles involved in accidents resulting in frame damage, major body or sheet metal damage, or where the steering column has been impacted, or where supplemental inflatable restraint systems deployed may also have a damaged or misaligned steering column.

• |
- Check the capsules on the steering column bracket assembly for any loose conditions when pushing or pulling by hand.

- | If the capsules are not securely seated and the bracket is bolted to the jacket assembly, replace only the bracket.

- | If the capsules are not securely seated and the bracket is welded to the jacket assembly, replace only the jacket assembly.

• |
- Check for jacket assembly collapse by measuring the distance from the lower edge of the upper jacket to a defined point on the lower jacket. Replace the jacket assembly if the measured dimensions are not within specifications.

• |
- Visually inspect steering shaft for sheared injected plastic (1). If steering shaft shows sheared plastic, replace the steering shaft.

• |
- Check steering shaft runout for any frame damage that could cause a bent steering shaft. Using a dial indicator at the lower end of the steering shaft, rotate the steering wheel. The runout must not exceed 1.59 mm (0.0625 in).