For 1990-2009 cars

# November, 1999 Labor Time Guide Updates

Subject: | November, 1999 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - G Van Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96-F | 96-1 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | T | V | W | X | Y
GRILLE ASSEMBLY - REPLACE

- PART GP: 1.266

- INC: Transfer trim and all fasteners

N

ONE PIECE | R | B1308 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
COMPUTER (CONTROL), BODY - REPLACE

- INC: Time to program new module

N

N4800

--

--

--

--

--

--

0.5

ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

--

0-.3

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SENSOR, YAW RATE - REPLACE | R | H2582 | -- | -- | -- | 0.7 | 0.8 | 0.8 | 0.8
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SUNSHADE, AUXILIARY - R&R OR REPLACE

- PART GP: 10.225

RIGHT | R | C2028 | 0.2 | 0.2 | 0.2 | 1.6 | 1.6 | 1.6 | 0.2
LEFT | R | C2029 | 0.2 | 0.2 | 0.2 | 1.6 | 1.6 | 1.6 | 0.2
ANTENNA COMPONENTS - REPLACE

- PART GP: 9.645

ESCUTCHEON/GUIDE | R | R0410 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 |
POWER |  |  |  |  |  |  |  |  |
MAST | R | R0420 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 |
POWER |  |  |  |  |  |  |  |  |
LEAD-IN | R | R0440 | 0.2 | 0.2 | 0.2 | 0.7 | 0.7 | 0.7 | 0.7
POWER |  |  |  |  |  |  |  |  |
COMPLETE ASSEMBLY | R | R0480 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 |
No Change to "ADD" Condition
*IND: N - New/R - Revised

#### LTG Update - Medium Duty Platform

OPERATION | IND* | OP NUM | CAB STYLE YEAR VIN CODE
--- | --- | --- | ---
B | A/W5 | C | H
NOTE: THE A445 TRANSMISSION, AS LISTED THROUGHOUT THIS GUIDE, WILL NOW BE REFERENCED AS AISIN 450 |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
GEAR ASSEMBLY, POWER STEERING - R&R

- PART GP: 6.508

- INC: Adjust gear

- NOTE: For check and adjust toe-in, refer to Operation E2000 and add the applicable times to the regular hours column

R

E9720

ACHIEVA & SKYLARK |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 |  |
GRAND AM & ALERO |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.4 | 1.4
MALIBU & CUTLASS |  |  | -- | -- | -- | 1.7 | 1.7 | 1.7 | 1.7
ADD:

- A- To Replace Grommets

0.1

0.1

0.1

0.1

0.1

0.1

0.1

B- To Replace Stub Shaft Seals | R |  | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
C- To Recondition P/S Gear (Complete) |  |  | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BRACKET, FUEL VAPOR CANISTER MOUNTING - REPLACE

- POLICY: E

R

L0600

AUTOMATIC |  |  | 0.3 | 0.3 | 0.3 | 1.8 | 1.8 | 1.8 | 1.8
MANUAL |  |  | 0.3 | 0.3 | 0.3 | 1.6 | 1.6 | 1.6 | 1.6
CANISTER, FUEL VAPOR - REPLACE

- PART GP: 3.130

- POLICY: E

R

L0620

AUTOMATIC |  |  | 0.4 | 0.4 | 0.4 | 1.7 | 1.7 | 1.7 | 1.7
MANUAL |  |  | 0.4 | 0.4 | 0.4 | 1.5 | 1.5 | 1.5 | 1.5
*IND: N - New/R - Revised