For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Windshield washer solvent level indicator is always ON.
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the windshield washer solvent level switch connector.
2. Turn ON the ignition switch.
3. Use a DMM in order to measure the voltage at harness connector terminal B.

Is the voltage within the specified range?

B+

Go to Step 3

Go to Step 4

3 | With the DMM set to the ohms scale, measure the resistance of the ground circuit (harness connector terminal A). Is the resistance within the specified range? | 0-5 ohms | Go to Step 5 | Go to Step 6
4 | Locate and repair an open in circuit XB3. Did you find and repair a circuit problem? | -- | Go to Step 8 | Go to Step 7
5 | Replace the windshield washer solvent level switch. Is the replacement complete? | -- | Go to Step 8 | --
6 | Locate and repair an open ground circuit. Is the repair complete? | -- | Go to Step 8 | --
7 | Replace the gauge cluster. Is the replacement complete? | -- | Go to Instrument Cluster System Check | --
8 |

1. Connect all connectors and components that you previously removed.
2. Test the low windshield washer solvent level indicator.

Does the low windshield washer solvent level indicator operate properly?

--

System OK

Go to Step 2