For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Remove the air inlet grille Refer to Air Inlet Grille Panel Replacement in Body Front End.
3. Press the nozzle retaining tabs together in order to remove the nozzle from the air inlet grille.
4. Remove the nozzle (1) from the air inlet grille.
5. Remove the hose from the nozzle (1).

### Installation Procedure

1. Install the hose to the nozzle (1).
2. Install the nozzle to the air inlet grille ensuring the nozzle retaining tabs lock into place.
3. Install the air inlet grille Refer to Air Inlet Grille Panel Replacement in Body Front End.
4. Close the hood.