For 1990-2009 cars

### Removal Procedure

The LH duct and RH duct temperature sensors are located in the HVAC module just above where the floor air outlets connect to the module.

Caution: Refer to SIR Handling Caution in the Preface section.

1. Remove the sound insulator (driver side shown).
2. Remove the front floor air outlet from the HVAC module.
3. Turn the temperature sensor (1) 180 degrees.
4. Carefully remove the temperature sensor from the air distribution module.
5. Disconnect the electrical connector from the temperature sensor.

### Installation Procedure

1. Connect the electrical connector to the temperature sensor.
2. Carefully insert the temperature sensor into the air distribution module.
3. Turn the temperature sensor (1) 180 degrees.
4. Install the front floor air outlet.
5. Install the sound insulator (driver side shown).