For 1990-2009 cars

### Removal Procedure

With a small flat-bladed tool pry on the side of the traction control switch and remove the switch from the instrument panel (I/P) accessory trim panel.

This will disengage the traction control switch from the electrical connector.

### Installation Procedure

1. Align the traction control switch with the electrical connector in the I/P accessory trim plate.
2. Push inward on the traction control switch until fully seated in the I/P accessory trim plate.

This will engage the electrical connector to the traction control switch.