For 1990-2009 cars

### Removal Procedure

Important: The rear headrest restraints are not serviceable.

1. Release the tabs located under the headrest restraint by pushing in.
2. Remove the headrest restraint by pulling out.

### Installation Procedure

1. Align the headrest restraint supports with the release tabs and push into place.
2. Pull out the headrest restraint in order to ensure that the restraint stops at detent.
3. Install the headrest restraint to the original position.