For 1990-2009 cars

# Warranty Admin. - December, 2000 Labor TIme Guide Updates

Subject: | December, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

#### LTG Update - All Applicable Platforms

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CONVERTER, OXIDATION CATALYTIC - REPLACE

- PART GP: 3.685

- POLICY: E (7/70 California - Includes other applicable states)

- POLICY: E (8/80 U.S. & 8/130 CANADA)

L2300

--

--

--

0.6

0.6

0.6

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MOTOR AND/OR FAN, BLOWER - R&R OR REPLACE

- NOTE: No Change to "PART GP", or Labor Operations D1321 and D1325

HEATER (NON A/C) |  | D1320 |  |  |  |  |  |

- GAS ENGINE

R

0.6

0.6

0.6

0.6

0.6

0.6

- DIESEL ENGINE

0.6

0.6

0.6

0.6

0.6

0.6

- A/C

D1322

- GAS ENGINE

R

0.6

0.6

0.6

0.6

0.6

0.6

- DIESEL ENGINE

0.6

0.6

0.6

0.6

0.6

0.6

- RIGHT HAND DRIVE

--

--

1.0

1.0

1.0

- No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - C/K - New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
HOUSING ASSEMBLY, SUNROOF - REPLACE |  | B2780 | -- | -- | -- | -- | 2.1 | 2.1
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
HARNESS, WHEEL SPEED SENSOR JUMPER WIRING (ABS) - REPLACE

- NOTE: No Change to "NOTE" or Labor Operation H2537

FRONT |  |  |  |  |  |  |  |
RIGHT | R | H2530 | 0.3 | 0.3 | 0.3 | 0.3 | -- | 0.7
LEFT | R | H2531 | 0.3 | 0.3 | 0.3 | 0.3 | -- | 0.7
BOTH | R | H2532 | 0.4 | 0.4 | 0.4 | 0.4 | -- | 1.0

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
BODY, COMPLETE

- NOTE: No Change to Labor Operation A5440

COLOR/CLEAR COAT |  | A5435 |  |  |  |  |  |

- PONTIAC

16.4

16.4

16.4

16.4

16.8

16.8

| R |  | KG | KG | KG | KG | KG | KG

- OLDSMOBILE

14.5

14.5

14.5

14.5

|  |  | JO | JO | JO | JO |  |

- BUICK

R

14.8

14.8

14.8

14.8

15.8

15.8

| R |  | JN | JN | JN | JN | JH | JH

- No Change to "ADD" Conditions

ANTENNA COMPONENTS - REPLACE

- NOTE: No Change to "PART GP", "NOTEs", or Labor Operations R0220 thru R0514

MODULE | R | R0520 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4

- No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SENSOR, LOW TIRE PRESSURE WARNING - REPLACE

- INC: Program sensor

FRONT |  |  |  |  |  |  |  |
RIGHT | N | E0720 | -- | -- | -- | -- | -- | 0.6
LEFT | N | E0721 | -- | -- | -- | -- | -- | 0.6
REAR |  |  |  |  |  |  |  |
RIGHT | N | E0724 | -- | -- | -- | -- | -- | 0.6
LEFT | N | E0725 | -- | -- | -- | -- | -- | 0.6
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | -- | -- | -- | -- | -- | 0-0.3
*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SENSOR, LOW TIRE PRESSURE WARNING - REPLACE

- INC: Program sensor

FRONT |  |  |  |  |  |  |  |
RIGHT | N | E0720 | -- | -- | -- | -- | -- | 0.6
LEFT | N | E0721 | -- | -- | -- | -- | -- | 0.6
REAR |  |  |  |  |  |  |  |
RIGHT | N | E0724 | -- | -- | -- | -- | -- | 0.6
LEFT | N | E0725 | -- | -- | -- | -- | -- | 0.6
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | -- | -- | -- | -- | -- | 0-0.3
SWITCH - REPLACE

- NOTE: No Change to "NOTEs", "INCs" or Labor Operations N2110 thru N2330 or N2384 thru N2610

PARKING BRAKE LAMP | R | N2380 | 0.3 | 0.3 | 0.3 | 0.3 | 0.6 | 0.6

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PLUGS, SPARK - REPLACE

- PART GP: 2.270

ONE | R | J4226 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3

- No Change to "ADD" Conditions

CONVERTER, OXIDATION CATALYTIC - REPLACE

- NOTE: No Change to "PART GP" or "POLICIES"

L2300

- M VAN

0.8

0.8

0.8

0.8

0.8

0.8

- L VAN

R

0.9

0.9

0.9

0.9

0.9

0.9

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
DOOR (VALVE), MODULE - REPLACE

- NOTE: No Change to "INC", "PART GP", or Labor Operations D1860, D1870 or D1877

UPPER AND/OR LOWER MODE |  | D1867 |  |  |  |  |  |

- MALIBU & CUTLASS

--

2.8

2.8

2.8

2.8

2.8

- ACHIEVA & SKYLARK

1.5

1.5

1.5

- GRAND AM & ALERO

R

1.5

1.5

1.5

5.1

5.1

5.1

- No Change to "ADD" Condition

MANIFOLD AND/OR GASKET, INTAKE LOWER - R&R OR REPLACE

- NOTE: No Change to "PART GP", "POLICY" or "NOTE"

- Applies to V6 Engine, Codes M, E and J

J0224

- MALIBU & CUTLASS

--

4.2

4.2

4.2

4.2

4.2

- ACHIEVA & SKYLARK

4.2

4.2

4.2

- GRAND AM & ALERO

4.2

4.2

4.2

4.4

4.4

4.4

ADD: |  |  |  |  |  |  |  |
A- To Replace Lower Manifold |  |  | 0.3 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
B- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec |  |  | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
C- With Secondary Air Injection | N |  | -- | -- | -- | 0.3 | 0.7 |
*IND: N - New/R - Revised

#### LTG Update - S Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MODULE, PCM/VCM - REPLACE

- NOTE: No Change to "POLICY" or "INC"

R

J6360

1.2

1.2

0.9

0.9

0.7

0.7

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SHOE, REAR DISC PARKING BRAKE - REPLACE | N |  |  |  |  |  |  |
RIGHT |  | H3050 | -- | -- | -- | 0.6 | 0.6 | 0.6
LEFT |  | H3051 | -- | -- | -- | 0.6 | 0.6 | 0.6
BOTH |  | H3052 | -- | -- | -- | 0.8 | 0.8 | 0.8
INJECTOR, SEQUENTIAL CENTRAL PORT FUEL - REPLACE

- POLICY: E

- INC: One or All Injectors

N

ONE | R | J5550 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
ADD: |  |  |  |  |  |  |  |

- A- To Replace Additional Injector(s) - One or All (NOTE: THIS "ADD" CONDITION HAS BEEN DELETED)

R

B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MODULE, SIDE IMPACT INFLATOR (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM) - R&R OR REPLACE

- INC: Disable and Enable SIR System

DRIVER (POWER) | N | C8856 |  |  |  |  |  |

- CHEVROLET

- IMPALA

--

--

--

--

0.6

0.6

- MONTE CARLO

--

--

--

--

0.7

0.7

- BUICK

- REGAL

--

--

--

--

0.6

0.6

ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | -- | -- | -- | -- | 0-0.3 | 0-0.3
B- With heated seats (Buick only) |  |  | -- | -- | -- | -- | 0.1 | 0.1
COVER AND/OR GASKET, TIMING - REPLACE

- PART GP: 0.206

- NOTE: Applies to V6 Engine, Codes M, T, J and E

J0780

- EXC CHEVROLET LUMINA

R

4.2

4.2

4.2

4.2

4.2

4.2

- CHEVROLET LUMINA

R

5.5

5.5

5.5

5.5

5.5

5.5

- No Change to "ADD" Condition

RESISTOR, FUEL PUMP - REPLACE

- NOTE: Applies to Engine Code 1 only

N

J5612

0.3

0.3

1.3

1.3

1.3

ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 |
COVER AND/OR GASKET, VALVE BODY - REPLACE

- NOTE: Applies to Auto Trans 4T65E

- NOTE: No Change to "PART GP" or "NOTE"

K5640

- ENGINE CODE K, E, J, M (MONTE CARLO/IMPALA)

R

--

2.8

2.9

2.9

3.1

3.1

- ENGINE CODE K, 1, J, M (EXC MONTE CARLO/IMPALA)

--

2.8

2.9

2.9

2.9

2.9

- ENGINE CODE X

--

3.5

- ENGINE CODE H

--

--

--

3.5

3.5

3.5

SOLENOID, PRESSURE CONTROL - REPLACE

- NOTE: Applies to Auto Trans 4T65E

R

K6353

--

2.8

3.2

3.2

3.3

3.3

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
REGULATOR, FRONT DOOR WINDOW - R&R OR REPLACE

- NOTE: No Change to "PART GP", "INCs", or "NOTE"

RIGHT POWER |  | C0182 | 0.8 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
LEFT POWER |  | C0183 | 0.8 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised