For 1990-2009 cars

### Removal Procedure

1. Remove the rear license plate lamp screws from the rear fascia.
2. Remove the rear license plate lamp from the rear fascia.
3. Disconnect the electrical connectors from the license plate lamp.
4. Remove the protective boot retaining plate (1) from the license plate lamp.
5. Remove the rubber protective boot (2) to reveal the bulb.
6. Remove the license plate bulb from the license plate lamp.

### Installation Procedure

1. Install the license plate bulb to the license plate lamp.
2. Install the rubber protective boot (2) over the bulb.
3. Install the retaining plate (1) to secure the boot.
4. Connect the electrical connectors to the license plate lamp.
5. Install the rear license plate lamp to the rear fascia.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the rear license lamp screws to the fascia.

Tighten
Tighten the rear license lamp screws to 2 N·m (18 lb in).