For 1990-2009 cars

#### Automatic Transmission Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BLU | FP723 | Transmission Position Signal
B | BLK/GRN | FU726 | Transmission Position Signal
C | BLK/YEL | FB708 | Transmission Position Signal
D | BRN | X756 | B+ from Fuse #3
E | BLK/RED | FA501 | Starter Solenoid Signal
F | WHT/BLK | MF757 | Rear View Mirror Signal
G | GRY | R733 | Transmission Position Signal
H | BLK/RED | FA500 | B+ in the ON Position

#### Gauge Cluster Connector

Connector Part Information |

• | ZF 26-1

• | 26 Way F

• | YEL

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/YEL | XB3 | WSWA Solvent Level Signal
2 | YEL/RED | BA2 | Brake Pad Wear Signal
3 | BRN/BLU | XP2 | Coolant Level Signal
4 | BRN/GRN | XU600 | Oil Level Signal
5 | RED | A900 | B+ from Fuse #24
6 | BLK | F8 | Ground to G103
7-8 | -- | -- | Not Used
9 | BLU/RED | PA600 | Vehicle Speed Signal
10-12 | -- | -- | Not Used
13 | GRN | U5 | Tachometer Signal
14 | BRN/BLK | XF20 | Seat Belt Signal
15 | BLU/GRN | PU1 | Oil Pressure Signal
16 | GRY/WHT | RM900 | Headlamp Switch Signal
17 | GRY/YEL | RB103 | Interior Lamps Dimming Signal
18 | BLU/WHT | PM1 | Generator Signal
19 | -- | -- | Not Used
20 | BRN | X70 | B+ from Fuse #15
21 | BRN/PPL | XY2 | ALC Sensor Signal
22 | RED | A16 | Ground Signal
23 | BRN/BLU | XP840 | Security Lamp Indicator
24 | BLK | F11 | Ground to G103
25 | -- | -- | Not Used
26 | BLU/YEL | PB90 | Oil Pressure Sensor Signal

#### Ignition Switch and Lifting Magnet

Connector Part Information |

• | ZF7-5

• | 7 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A905 | B+ from Fuse #24
2 | GRN | U900 | Brake to Shift Signal
U | BRN | X826 | B+ in the ON Position
V | BRN | X1 | B+ in the ON or START Position
W | RED | A19 | B+ when the Key is inserted
Y | RED | A503 | B+ Fused
Z | BLK/RED | FA700 | Starter Solenoid Signal