For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion.

Pull the release handles which are located at the base of rear seat cushion.

2. Disconnect the heating element electrical connectors (1) from the rear seat cushion.
3. Remove the rear seat belt from the lower seat cushion.
4. Remove the rear seat cushion from the vehicle.

### Installation Procedure

1. Install the rear seat cushion to the vehicle.
2. Install the rear seat belt to the lower seat cushion.
3. Connect the heating element electrical connectors (1) to the rear seat cushion.
4. Install the rear seat cushion.

Insert the rear seat cushion to the inner floor pan. Push downward in order to lock the cushion into place.