CHECKING CORRECT FLUID LEVEL INDICATOR LOCATION / TRANSAXLE. Cadillac Cimarron 1987

For 1990-2009 cars

# CHECKING CORRECT FLUID LEVEL INDICATOR LOCATION / TRANSAXLE

#### MODELS AFFECTED: 1987 CIMARRON EQUIPPED WITH (MG282) 5-SPEED TRANSAXLE

The (MG282) Manual 5-Speed Transaxle for the 1987 Cimarron is equipped with a fill tube. This is not to be confused with the level indicator and fluid fill tube used with other transaxles which is similar in appearance.

The (MG282) 5-Speed Manual Transaxle has a fluid indicator that screws into the case showing the required fluid level when checked using the correct procedures (see Figures I and 2).

If a fill tube plug has been replaced with an incorrect level indicator, it should be replaced with the correct plug (see Figure 3). This will also result in an overfill condition (see Figure 4) accompanied by high shift effort (hard shifting).

Part Number Description ----------- ----------- 10046677 Plug Transmission Lube Fill - MG282

Check the transaxle fluid level and adjust as required using the correct (screw-in type) level indicator.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.