1986 MODEL PAINT CHARTS SUPPLIERS & REPAIR PROCEDURES. Cadillac Cimarron 1986

For 1990-2009 cars

# 1986 MODEL PAINT CHARTS SUPPLIERS & REPAIR PROCEDURES

#### SUBJECT: 1986 MODEL PAINT INFORMATION

The listings of 1986 paint codes contained in this bulletin will enable dealers to order the necessary paint materials required for effective field repairs.

The list of colors indicates the suppliers' ordering codes for exterior, interior, vinyl roof moldings, and paint stripe colors.

Listed below is a current listing of the various Cadillac Assembly Plants and their suppliers. It should be noted, however, that paint suppliers are subject to change.

Assembly Plant Paint Type Paint Supplier Paint Codes -------------- ---------- -------------- ----------- Fleetwood Dispersion Lacquer Inmont All

Hamtramck B/C C/C Enamel DuPont Ail

Orion B/C C/C Ersamel PPG All

Janesville Dispersion Lacquer DuPont All

Other manufacturers produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

The paint listed in this bulletin is (or soon will be) available from local paint suppliers.

EXTERIOR PLASTIC PARTS

All 1996 Cadillacs have exterior parts made of various types of plastic materials that require specific procedures to obtdin high quality refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1986 models. For best results when painting is required, determine the type of plastic material from the chart. Then follow the correct point procedure, depending upon what painting material and equipment is available.

PLASTIC TYPE SYMBOL

Therrmoset Urethane RRIM Thermoplastic Urethare TPU Thermosetting Polyester UP(SMC) Thermoplastic Urethane RIM Thermoplastic Elastomer TPE

A. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM), Thermoplastic Elastomer (TPE), Thermoplastic Polyester (SMC), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to the manufacturer's literature available through your jobber for details on proper mixing and application.

1. Thoroughly clean part by washing with a suitable cleaning solvent* to remove all surface contaminates.

#### NOTICE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stipped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

2. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A.

#### NOTICE: Unpainted parts do not require sanding prior to painting, but should be thoroughly cleaned as in Step 1.

3. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding. (For most products, approximately 30 minutes).

4. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes flash time between each double coat and allow to completely dry before using.

5. Following is a list of some of the products available for painting flexible plastic.

Ditzler Elastomeric Primer - DPXS44 Ditzler Flexative - DX369 (Permanent Flexible Urethane Additive) Ditzler Flex Additive - DX1798 (Non-Urethane Additive) Ditzler Delthane - DXR80 (Acrylic Enamel Hardner) Rinshed-Mason Acrylic Flex Agent 891 DuPont Dexlar Flexible Finish (Lucite tints plus Dexlar 365B Additive) Sherwin-Williams Flex Additive - V2V297 Acme/Rogers Flex Additive - 699/4699 Martin-Senour Flex Additive - 3082

*Cleaning Solvents

a. DuPont Prep-Sol b. Rinshed-Mason Pre-Kleano 900 c. Ditzler Acryli-Clean DX330 d. Sherwin-Williams R7K156 e. Acme 88; Rogers 088 f. Martin-Senour 6383

B. NYLON - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

C. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required; paint with acrylic lacquer.

D. POLYESTER PARTS (UP, PBTP) - Will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

E. POLYPROPYLENE - Interior parts.

1. Wash surface thoroughly with enamel reducer. (Do not use wax and grease removers.)

2. Apply primer immediately and allow to dry completely before color coating.

3. Color coat with lacquer or enamel reduced and applied according to the manufacturerer's recommendation.

4. Materials:

Cleaning Solvent - DuPont 3812S Enamel Reducer Ditzler DTE-101 or DTE-102 "Bobcat" Enamel Reducer Primer - DuPont 3293 GM 1052364

1986 MODEL PAINT INFORMATION EXTERIOR -------- Paint Color Martin- Sherwin- Code Name WA# Dupont Ditzler Senour Williams R-M # ---- ----- --- ------ ------- ------ --------- ----- 08 M. K. Pink 7795 2304 70748 99-6081 34/35-3442 12899 11 Cotillion White 3967 5338 2058 30-3929 L10A2864 2080 5644 12 Silver Met. 8535 B8501 3746 30-5371 34380 15001 13S Silver Met. 9021 D8590 3822 30-5491 35369 15365 15 Med. Gray Met. 8573 B8502 3749 30-5372 34381 15004 19 Sable Black 848 99S 9300 3069 L10B1738 A946 3000/4590 22 Lt. Blue Met. 8533 B8538 3753 30-5374 34383 15008F 25 Lt. Blue Met. 8574 B8503 3754 30-5373 34382 15009 29 Dk. Blue Met. 8540 B8547 3757 30-5376 34385 15011D 31 Dk. Blue Met. 8592 B8504 3760 30-5441 34875 15014 38 Sungold 8758 B8611 3887 30-5522 35314 16005D 40 White 8554 B8469 3680 30-5295 33755 13570 41 Black 8555 99S 9700 30-5296 33756 13572 43 Lt. Sage Met. 8572 B8505 3762 30-5377 34386 15016 46 Med. Sage Met. 8569 B8506 3763 30-5379 34388 15017 48 Black Emerald Met. 8747 BB608 3888 30-5482 35315 16006 64 Yellow Beige 8525 B8521 3769 30-5437 34861 15023 55 Chamois 8564 B8615 3890 30-5384 34393 160080 57 Dk. Sandstone Met. 8543 B8514 3771 30-5386 34395 15025D 58 Lt. Chestnut Met. 8575 B8587 3772 30-5387 34396 15026 63 Lt. Driftwood 8744 B8603 3894 30-5481 35310 16011 65 Med. Driftwood Met. 8745 B8604 3895 30-5483 35317 16012F 73 Lt. Maple Met. 8491 B8108 3331 30-4988 31055 13522V 74 Flame Red Met. 8748 B8610 3823 30-5485 35320 16017 75 Garnet Red Met. 8746 B8606 3900 30-5477 35278 16018 77 Dk. Russet Met. 8599 B8515 3784 30-5394 34403 15038F 79 Dk. Red Met. 8529 B8509 3786 30-5396 34405 15040M 80 Sandstone 8538 B8513 3770 30-5385 34394 15024 82 Dk. Grey F/M 8549 B8519 3793 30-5408 34420 15047 83 Canyon Red F/M 8544 B8522 3790 30-5400 34409 15044R 84 Gun Metal Met. 7782 B8403 3667 30-5313 33936 14066D 85 Med. Blue F/H 8541 B8520 3789 30-5399 34408 15043 86 Med. Quartz Met. 8761 B8614 3902 30-5527 35323 16020F 87 Lt. Sandstone F/M 8571 B8518 3787 30-5403 34412 15041 88 Dk. Gray Met. 8600 B8517 3788 30-5398 34407 15042 89 Autumn Maple F/M 8237 B8385 3532 30-5244 33074 13131V 90 White Diamond Met. 8933 B8609 3903 30-5528 35424 16021 91 Heather F/M 8539 C8401 3684 30-5356 34330 14077D 92 Med. Emerald F/M 8931 B8607 3904 30-5474 35255 16022G 93 Heather Met. 8597 B8516 3791 32-5401 34410 15045 94 Med. Blue F/M 8545 B8549 3792 30-5402 34411 15046D 95 Sungold F/M 8759 B8612 3905 30-5478 35279 16023F 96 Dk. Driftwood F/M 8765 B8605 3906 30-5486 35324 16024G 97 Lt. Quartz F/M 8760 B8613 3907 30-5529 35325 16025G 98 Chamois F/M 8565 B8616 3908 30-5404 34413 16026D 99 Black Chery Met. 8244 B8414 3673 30-5337 33941 14071D

1986 MODEL PAINT INFORMATION INTERIOR --------

Paint Color Ditzler Ditzler Ditzler Code Name WA # DUPONT Low Gloss Semi-Gloss UCV ---- ---- ---- ------ --------- ---------- ------- 11N White 3835 C8622-5 deg. -- 90233 -183 C8536-12 deg. 19N Black 848 4428-5 deg. -- 9433 -120 C8535-12 deg.

27CN Dark Blue 8576 C8562-5 deg. -- 15886 2-1098 C8439-12 deg. 488N Med. Emerald 8796 C8621-5 deg. -- 45898 2-1165 C8614-12 deg. 48DN Dark Emerald 8788 C8660-5 deg. -- 45890 2-1166 C8661-12 deg. 50AN Light Yellow 7042 C8388-5 deg. -- 82563 2-580 C8365-12 deg. 50BN Dark Yellow 8803 C8662-56 deg. 82658 82659 2-1177 C8663-12 deg. 50CN Very Dk Yellow 8804 C8664-5 deg. -- 82631 2-1168 C8665-12 deg. 52AN Chamois 8580 C8565-5 deg. -- 25500 2-1102 C8365-12 deg. 52BN Lt. Chamois 8584 C8666-5 deg. -- 25501 2-1119 C8545-12 deg. 52CN Dark Chamois 8585 C8568-5 deg. 25569 25502 2-1120 C8553-12 deg. 60AN Lt. Driftwood 8782 C8623-5 deg. -- 25644 2-1169 C8615-12 deg. 60BN Med. Driftwood 8802 C8667-5 deg. 25777 25778 2-1178 C8668-12 deg. 60CN Dk. Driftwood 8790 C8673-5 deg. -- 25648 2-1170 C8674-12 deg. 62AN Light Saddle 7769 C8590-5 deg. -- 25230 2-1025 C8352-12 deg. 62CN Dark Saddle 8613 C8669-5 deg. 25570 25503 2-1126 C8551-12 deg. 68CN Russet 8579 C8564-5 deg. -- 25513 2-1101 C8542-12 deg. 69BN Med. Beige 8248 C8557-5 deg. -- 25313 2-1045 C8446-12 deg. 69CN Dark Beige 8280 C8561-5 deg. 25571 25514 2-1117 C8554-12 deg. 72CN Carmine 8577 C8563-5 deg. -- 72800 2-1172 C8540-12 deg. 78CN Garnet Red 8781 C8624-5 deg. -- 72799 2-1173 C8616-12 deg. 79CN Claret 4887 C8624-5 deg. 51085 51170 2-479 C8616-12 deg. 82CN Med Dark Gray 8247 C8556-5 deg. 33873 33665 2-1048 C8447-12 deg. 82DN Dark Gray 8595 C8597-5 deg. 33874 33824 2-1125 C8550-12 deg. 94BN Light Quartz 8783 C8625-5 deg. -- 51184 2-1174 C8617-12 deg. 94CN Dark Quartz 8795 C8670-5 deg. -- 51189 2-1175 C8671-12 deg. 99DN Black Cherry 8249 C8558-5 deg. -- 72575 2-1049 C8540-12 deg.

Paint Color Martin- Sherwin-Williams R-H Code Name WA # Senour ACME/Rogers Inmont ---- ---- ---- ------- ----------- ------- 11N White 3835 32-17172-5 deg. 35574-5 deg. 4402-5 deg. 32-17029-12 deg. 33777-12 deg. 19N Black 848 32-16615-5 deg. J4-8677-5 deg. 12812-5 deg. 32-16918-12 deg. 92387-5 deg. 4401-12 deg. 33024-12 deg. 27CN Dark Blue 8576 32-17075-5 deg. 34606-5 deg. 16045-5 deg. 32-17067-12 deg. 34598-12 deg. 15080-12 deg. 488N Med. Emerald 8796 32-17140-5 deg. 35439-5 deg. 32-17131-12 deg. 35430-12 deg. 16059-12 deg. 48DN Dark Emerald 8788 32-17137-5 deg. 35436-5 deg. 32-17149-12 deg. 35470-12 deg. 16047-5 deg. 50AN Light Yellow 7042 32-16992-5 deg. 32351-5 deg. 32-17030-12 deg. 33778-12 deg. 9558-12 deg. 50BN Dark Yellow 8803 32-17154-5 deg. 35475-5 deg. 32-17133-12 deg. 35432-12 deg. 16062-12 deg. 50CN Very Dk Yellow 8804 32-17141-5 deg. 35440-5 deg. 32-17152-12 deg. 35473-12 deg. 16050-5 deg. 52AN Chamois 8580 32-17077-5 deg. 34608-5 deg. 32-17069-12 deg. 34600-12 deg. 15088-12 deg. 52BN Lt. Chamois 8584 32-17125-5 deg. 35041-5 deg. 32-17124-12 deg. 35040-12 deg. 15267-12 deg. 52CN Dark Chamois 8585 32-17082-5 deg. 34613-5 deg. 32-17070-12 deg. 34601-12 deg. 15094-5 deg. 60AN Lt. Driftwood 8782 32-17135-5 deg. 35434-5 deg. 32-17129-12 deg. 35428-12 deg. 16056-12 deg. 60BN Med. Driftwood 8802 32-17153-5 deg. 35474-5 deg. 32-17132-12 deg. 35431-12 deg. 16061-12 deg. 60CN Dk. Driftwood 8790 32-17138-5 deg. 35437-5 deg. 32-17150-12 deg. 35471-12 deg. 16048-5 deg.

62AN Light Saddle 7769 32-17086-5 deg. 34729-5 deg. 13180-12 deg. 32-16912-12 deg. 32996-12 deg. 16043-5 deg. 62CN Dark Saddle 8613 32-17081-5 deg. 34612-5 deg. 15096-5 deg. 32-17072-12 deg. 34603-12 deg. 16053-12 deg. 68CN Russet 8579 32-17087-5 deg. 34759-5 deg. 32-17068-12 deg. 34599-12 deg. 15087-12 deg. 69BN Med. Beige 8248 32-16966-5 deg. 33770-5 deg. 16071-5 deg. 32-16950-12 deg. 33715-12 deg. 14006-12 deg. 69CN Dark Beige 8280 32-17074-5 deg. 34605-5 deg. 15065-5 deg. 32-17066-12 deg. 34597-12 deg. 16070-12 deg. 72CN Carmine 8577 32-17076-5 deg. 34607-5 deg. 16046-5 deg. 32-17085-12 deg. 34639-12 deg. 15084-12 deg. 78CN Garnet Red 8781 32-17134-5 deg. 35433-5 deg. 32-17147-12 deg. 35468-12 deg. 16055-12 deg. 79CN Claret 4887 32-17134-5 deg. 35433-5 deg. 12818-5 deg. 32-17084-12 deg. 34638-12 deg. 8763-12 deg. 82CN Med Dark Gray 8247 32-16965-5 deg. 33769-5 deg. 14088-5 deg. 32-16949-12 deg. 33714-12 deg. 14009-12 deg. 82DN Dark Gray 8595 32-17080-5 deg. 34611-5 deg. 15095-5 deg. 32-17071-12 deg. 34602-12 deg. 15268-12 deg. 94BN Light Quartz 8783 32-17136-5 deg. 35435-5 deg. 32-17130-12 deg. 35429-12 deg. 16057-12 deg. 94CN Dark Quartz 8795 32-17139-5 deg. 35438-5 deg. 32-17151-12 deg. 35472-12 deg. 16049-5 deg. 99DN Black Cherry 8249 32-16967-5 deg. 33771-5 deg. 32-17043-12 deg. 33791-12 deg. 14010-12 deg.

#### 1986 CADILLAC VINYL ROOF MOLDING COLORS

GM Sherwin- Paint Color Fisher R-M Martin- Williams Code Name "WA" No. Inmont DuPont Ditzler Senour ACME/Rogers ---- ---- -------- ------ ------ ------- ------ ----------- 11T White 8936 16110 C8659 2-130 32-26851 35781 11T White 3967 4415 D8369 2-130 32-26185 J4-5676 11510 13T Silver Met. 7781 14039 C8480 2-1052 32-26704 34123 19T Black 848 4416 D8368 -120 32-16082 J4-1990 9739 31T Dk. Blue Met. 8592 15060 D8556 2-1114 32-26753 35026 34T Lt. Blue Met. 8533 15061 D8555 2-1107 32-26754 35027 38T Sungold 8758 16104 B8611 2-1158 32-26844 35774 43T Lt. Sage Met. 8572 15182 D8557 2-1113 32-26761 35087 47T Med. Sage Met. 8531 15062 D8558 2-1106 32-26764 35110 48T Black Emerald Met. 8747 16101 B8608 2-1186 32-26841 35771 54T Yellow Beige 8525 15184 D8559 2-1104 32-26763 35109 55T Chamois 8564 16095 C8526 2-1187 32-26832 35762 57T Dk. Sandstone Met. 8563 15185 D8562 2-1112 32-26769 35115 63T Lt. Driftwood 8744 16098 B8603 2-1188 32-26838 35768 6ST Med. Driftwood Met. 8745 16099 B8604 2-1189 32-26839 35769 74T Flame Red get. 8748 16102 B8610 2-1190 32-26842 35772 75T Garnet Red Met. 8746 16101 B8606 2-1191 32-26840 35770 79T Dk. Red Met. 8529 15187 D8561 2-1105 32-26760 35086 82T Dk. Gray Met. 8549 15192 D8566 2-1111 32-26768 35114 84T Gunmetal Met. 7782 14040 C8481 2-1053 32-26705 34124 86T Med. Quartz Met. 8761 16107 B8614 2-1193 32-26847 35777 89T Autumn Maple Met. 7384 12786 D8386 2-921 32-26560 32415 91T Heather Met. 8539 15189 D8563 2-1108 32-26765 35111 92T Med. Emerald Met. 8931 16109 B8607 2-1194 32-26850 35780 94T Med. Blue Met. 8545 15063 D8565 2-1110 32-26767 35113 95T Sungold Met. 8759 16105 B8612 2-1195 32-26845 35775 96T Dk. Driftwood Met. 8765 16108 B8605 2-1196 32-26848 35778 97T Lt. Quartz Met. 8760 16106 B8613 2-1197 32-26846 35776 98T Chamois Met. 8565 16096 C8553 2-1198 32-26833 35763 99T Black Cherry Met. 8244 14044 C8485 2-1058 32-26709 34128

#### 1986 CADILLAC PAINT STRIPE COLORS

GM Sherwin- Paint Color Fisher R-M Martin- Williams Code Name "WA" No. Inmont DuPont Ditzler Senour ACME/Rogers ---- ---- -------- ------ ------ ------- ------ ----------- 09A Lt. Quartz 8810 16075 C8644 72803 32-26777 35563 10A Bright Quartz 8811 16076 C8645 72818 32-26791 35665 11A White 3967 2080 5338 2058 32-3929 LlOA2864 5644

14A Lt. Gray 8670 15165 C8529 33856 32-26729 34869 18A Gunmetal 8291 14036 C8441 33750 32-26700 34102 19A Black 848 A946 99S 930O 3069 L10B1738 300014590 21A Lt. Blue 8658 15073 C8520 15891 32-26721 34863 26A Med. Mauve 8666 15070 C8528 51169 32-26739 34813 28A Dk. Blue 8659 15074 C8521 15892 32-26722 34864 37A Lt. Emerald 8809 16077 C8646 16081 32-26776 35562 38A Bright Emereld 8812 16078 C8647 45936 32-26778 35564 43A Lt. Sage 8661 15072 C8523 45842 32-26726 34866 47A Dk. Sage 8662 15075 C8524 45843 32-26727 34867 48A Black Emerald 8854 16079 C8648 45937 32-26782 35568 51A Sun Gold 8758 16080 B8611 25803 30-5522 35314 55A Gold 8589 15076 D8276 25509 32-26703 34105 56A Lt. Driftwood 8744 16081 B8603 25802 30-5481 35310 57A Dk. Driftwood 8808 16082 C8640 25774 32-26775 35561 60A Chamois 8564 15172 B8615 25484 32-26720 34862 63A Sandstone 7260 12224 B8105 3327 30-4985 31052 66A Orange 8002 9500 45261 60909 32-26 25455

67A DK. Brown 8001 9502 45260 25088 32-26336 J4-8727 25460 75A Red 4721 4518 43592 72128 32-26272 J4-7191 11892 76A Garnet Red 8852 16086 C8643 51211 32-26780 35566 79A Dk. Claret 8663 15071 C8525 51167 32-26728 34868

#### 1986 CADILLAC DE VILLE AND FLEETWOOD RUB STRIP COLOR

Paint Color Martin- Sherwin- R-M Code Name WA # Dupont Ditzler Senour Williams Imont ---- ---- ---- ------ ------- ------ -------- ----- -- Med. Gray Met. 9145-50 deg. C8672 34173 32-26855 36383 16088

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.