TAIL LAMP ASSEMBLY REMOVAL PROCEDURE. Cadillac Cimarron 1986

For 1990-2009 cars

# TAIL LAMP ASSEMBLY REMOVAL PROCEDURE

#### MODELS AFFECTED: 1986 CIMARRON

This bulletin revises the information described in the 1986 Body Service Manual (pages 7E-11 and 7E-12) for removing and replacing the tail lamp assembly on 1986 Cimarrons.

The following procedure should be used when removing and replacing the tail lamp assembly.

#### Removal

1. Remove two screws securing license plate to license plate pocket.

2. Remove lamp assembly to pocket attaching screws, (Figure 1, Item 2).

3. Remove upper outer license pocket attaching nut (Figure 1, Item 4).

4. Open rear compartment lid and remove rear compartment end panel trim.

5. Remove four tail lamp assembly attaching nuts, (Figure 1, Item 3).

6. Remove tail lamp assembly, (Figure 1, Item 1)

#### Installation

Reverse removal procedure.

For warranty purposes, use operation number N-1590 to replace Right Tail Lamp Assembly, N-1591 to replace Left Tail Lamp Assembly at 0.3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.