RATTLE/CLICK AT START-UP (SHIELD CONVERTER, NEW P/N). Cadillac Cimarron 1988

For 1990-2009 cars

# RATTLE/CLICK AT START-UP (SHIELD CONVERTER, NEW P/N)

#### MODELS AFFECTED: 1985-1988 CIMARRONS WITH 2.8L V-6

Owners of 1985-1988 Cimarrons equipped with 2.8L engine with automatic transmission may notice a rattling or clicking noise coming from the engine compartment. This noise is more apparent when the engine is cold and usually goes away as the engine warms up.

The noise may be due to a warped torque converter shield being contacted by the flywheel. A torque converter shield currently used on other models has been released for use on the 2.8L Cimarron.

To repair this condition install converter shield, P/N 10009088. Use three of the existing bolts removed from the vehicle for installation.

Parts are currently available from GMSPO

For warranty purposes use Labor Operation J1440 at .3 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.