REAR CAM COVER OIL LEAK IMPROVED SEAL AND COVER. Cadillac Cimarron 1985

For 1990-2009 cars

# REAR CAM COVER OIL LEAK IMPROVED SEAL AND COVER

#### VEHICLES AFFECTED: 1982-86 J CAR WITH LQ5 (VIN P), L46 (VIN G), LR9 (VIN B), L4 ENGINES (PASS.) 1983-84 S/T TRUCK WITH LQ2 (VIN Y) L4 ENGINE

An improved seal for the rear cam cover, kit p/n 10054590, is available to replace the RTV sealant and cover plate. The surface should be thoroughly cleaned and checked for flush plugs in the sealing area before installing the new cover, p/n 14090972, and gasket p/n 14090974.

Torque bolts to 8-14 Nm.

Use existing labor operation number and labor time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.