BROKEN A/C COMP. DISCH. PIPE INSTALL BRACKET AND CLAMP. Cadillac Cimarron 1985

For 1990-2009 cars

# BROKEN A/C COMP. DISCH. PIPE INSTALL BRACKET AND CLAMP

#### MODELS AFFECTED: 1985 AND 1986 CIMARRONS EQUIPPED WITH 2.0L ENGINES

Some 1985 and 1986 Cimarrons equipped with the 2.0L/L4 engine may experience a broken air conditioning compressor discharge pipe.

A bracket and clamp support kit, to prevent recurrence of the failure, is now available from GMWDD under part number 22535625.

The bracket can be installed by removing the compressor to bracket bolt and installing the new bracket and clamp as shown below.

For warranty purposes use labor Operation T6164 for .3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.