FRONT BRAKE NOISE NEW LINING P/N RELEASED. Cadillac Cimarron 1985

For 1990-2009 cars

# FRONT BRAKE NOISE NEW LINING P/N RELEASED

#### MODELS AFFECTED: 1982-1986 CIMARRONS

Some 1982-1986 Cimarrons may exhibit a condition of front brake noise. All Cimarrons use semi-metalic brake linings. Semi-metalic linings have many advantages over asbestos linings, however, they also produce more noise than the asbestos linings used on previous model vehicles. If concerns of front brake noise is encountered on 1982-1986 Cimarrons, the front brake linings can be replaced with 1987 Cimarron linings, P/N 12321424. The 1987 lining is made of a different material. The lining edge code, which is stamped in the lining material on the outside curved edge, can be used to identify the new material. It should read "DM 128FE."

For warranty purposes, use Labor Operation H0042 at .7 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.