WINDSHIELD WIPER CHATTER AND WIPEABILITY. Cadillac Cimarron 1987

For 1990-2009 cars

# WINDSHIELD WIPER CHATTER AND WIPEABILITY

#### SUBJECT: WINDSHIELD WIPER BLADE CHATTER/WIPEABILITY CONCERNS CAUSED BY CHANGE IN BLADE ANGLE - (INSTALL SPACER)

#### VEHICLES AFFECTED: 1982-91 "J" CAR

Some 1982-91 J car coupes and convertibles may experience driver side blade chatter and wipeability concerns.

#### IMPORTANT: Before doing any work, clean windshield and both blades with GM windshield cleaner, PN 1050011 or equivalent. Then, recheck wiper-washer operation. If problems persist after cleaning, follow the procedures in this bulletin.

#### CAUSE:

------- Some vehicles have a wiper housing mounting tolerance condition that changes the attack angle of the driver side blade assembly and can cause blade chatter and wipe problems.

#### CORRECTION:

------------ Install spacer, Package #22111290, over driver side linkage housing as shown in Figure 1. Make sure spacer is correctly oriented.

Install new screws provided finger tight, then torque evenly to 8 N.m (70 lbs.in).

#### NOTE: When reassembling cowl, make sure that washer hose is reconnected (and not pinched).

If an interference condition results between the wiper arm head casting and the cowl clearance hole, use a file to enlarge hole at interference point.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.