PULSE WIPER PHANTOM WIPE OXIDATION-WIPER SW.CONTACTS. Cadillac Cimarron 1984

For 1990-2009 cars

# PULSE WIPER PHANTOM WIPE OXIDATION-WIPER SW.CONTACTS

#### MODELS AFFECTED: 1984 CIMARRON

Some 1984 Cimarrons may experience a false (phantom) wipe when the wiper control is in the "OFF" position.

To correct this condition, install a new pulse wiper switch, P/N 7848195, for a standard column or P/N 7848196 for a tilt column. Refer to Section 3B3 of the 1984 Cimarron Service Manual for the proper removal and installation procedure of the wiper switch.

For warranty purposes, use labor Operation No. N2610 at .8 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.