INNER TIE ROD TO GEAR BOLT LOCK PLATE REPLACEMENT. Cadillac Cimarron 1985

For 1990-2009 cars

# INNER TIE ROD TO GEAR BOLT LOCK PLATE REPLACEMENT

#### MODELS AFFECTED: 1985 CIMARRON

The inner tie rod bolt lock plate on 1985 Cimarron steering gears has been changed from a tab-type lock plate to a push-on retainer type lock plate (Figure 1).

The new push-on lock plate may become damaged during removal and may not retain properly if reused. For this reason, the push-on type lock plate must be replaced with a new lock plate, GMWDD P/N 7836778, any time it is removed.

This new push-on type lock plate will be included in all future packages of GMWDD tie rods and center take-off short gears.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.