FUEL LINE KNOCK/HAMMERING REPLACE FUEL FEED PIPE. Cadillac Cimarron 1986

For 1990-2009 cars

# FUEL LINE KNOCK/HAMMERING REPLACE FUEL FEED PIPE

FUEL LINE KNOCK/HAMMERING, - REPLACE ENGINE FUEL FEED PIPE-EXPANSION CHAMBER ASSEMBLY

#### VEHICLES AFFECTED: 1986 CHEVROLET AND CADILLAC J-CARS W/2.8L V6 ----------------- (RPO LB6)

Some 1986 Chevrolet Cavalier and Cadillac Cimarron vehicles with 2.8L MPFI engines may exhibit, a light hammering/knocking type noise audible in the passenger compartment that may be noted in a cold start mode, and/or warm stabilized mode and is most apparent at engine idle.

This condition may be caused by pressure pulsations in the fuel system generated by fuel injector operation,resulting in hydraulic hammering in chassis fuel pipes.

Vehicles exhibiting this condition may be repaired by installation of a new engine fuel feed pipe - expansion chamber assembly, P/N 10100095, following the service procedure in this bulletin.

#### Service Procedure:

1. Disconnect negative battery cable and remove fuel tank filler cap.

2. Relieve pressure in fuel system following shop manual procedure.

3. Disconnect electrical connectors to Mass Air Flow (MAF), Idle Speed Control (ISC) and Throttle Position Sensor (TPS) sensors.

4. Remove air cleaner assembly and duct to throttle body as a unit.

5. Remove cross-over pipe heat shield (2 nuts, 3 screws).

6. Disconnect throttle body coolant hoses at coolant pipes.

7. Disconnect EGR transfer tube from EGR valve.

#### NOTICE: CARE MUST BE TAKEN TO INSURE TRANSFER TUBE IS NOT DISPLACED (BENT) FROM ITS INSTALLED POSITION. SUCH MOVEMENT COULD JEOPARDIZE PART INTEGRITY AND RESULT IN EXHAUST GAS LEAKAGE.

8. Disconnect plenum from intake manifold (8 bolts, 1 stud) and rotate up and rearward.

9. Identify and mark relationship of fuel feed hose to chassis fuel feed pipe. Disconnect fuel feed hose at chassis fuel feed pipe utilizing backup wrench.

#### NOTICE: FUEL FEED HOSE ASSEMBLIES ARE FORMED PARTS AND MUST BE REINSTALLED IN THE SAME POSITION THEY WERE IN PRIOR TO REMOVAL. TWISTING THE HOSE MAY ADVERSELY AFFECT ENGINE OPERATION AND/OR HOSE INTEGRITY.

10. Disconnect fuel feed pipe at fuel rail.

11. Remove stud retaining fuel feed/return pipe clip to cylinder head.

12. Remove engine fuel feed pipe and fuel feed hose as an assembly.

13. With new fuel feed pipe / expansion chamber, P/N 10100095, positioned next to removed fuel feed pipe and hose, identify and mark hose assembly position on new pipe assembly.

14. Disconnect fuel feed hose from feed pipe and connect to new feed pipe / expansion chamber assembly utilizing backup wrench. Torque fitting to 20- 34 N.m. insuring hose is maintained in position identified in previous step.

15. Remove intake manifold bolt indicated in Illustration.

16. Route new fuel feed pipe expansion chamber assembly and hose into position and insert into fuel feed/return pipe clip.

17. Hand start fuel feed pipe fitting at fuel rail and feed/return pipe clip stud.

18. Insert intake manifold bolt through expansion chamber bracket and position expansion chamber to insure clearance between intake manifold runners/expansion chamber (See Illustration) and torque intake manifold bolt to 18 -24 N.m.

19. Torque fuel feed pipe fitting at fuel rail to 20 - 35 N.m. and retaining clip stud to 27 - 41 N.m.

20. Reconnect fuel feed hose to chassis fuel feed pipe insuring position Identified in Step 9 is maintained and torque to 20-34 N.m. utilizing backup wrench on fitting.

21. Assemble plenum to intake manifold utilizing new gaskets at both the plenum to intake manifold and EGR valve to EGR transfer tube interface.

22. Torque plenum and EGR transfer tube fasteners to 23 - 29 N.m.

23. Assemble crossover pipe heat shield to engine.

24. Install air cleaner and duct.

25. Reconnect electrical connectors, battery and install fuel tank filler cap.

26. Start engine, check all connections for possible fuel or coolant leaks and correct as required.

Parts required for this installation are noted below and are available from CANSPO.

Description Part Number Quantity Required ----------- ----------- -----------------

Fuel Feed Pipe and Expansion Chamber Asm. 10100095 1

Plenum Gasket Kit 14084058 1

EGR Transfer Tube Gasket 14088263 1

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.