PRODUCTION BATTERY CHANGE STANDARD AND HEAVY DUTY. Cadillac Cimarron 1984

For 1990-2009 cars

# PRODUCTION BATTERY CHANGE STANDARD AND HEAVY DUTY

#### MODELS AFFECTED: 1984 CIMARRON

A production change in the battery capacity on 1984 Cimarrons was recently made, effective at B.C. No. 407952. This change affects both the standard battery and the heavy duty battery option (UA1). These changes are as follows:

Before B.C. 407952 Standard Battery Heavy Duty Option (UA1) ------------------ ---------------- ----------------------- Battery 70-60 75-60 Reserve Capacity 75 Minutes 90 Minutes Cold Cranking Amperage 405 Amperes 500 Amperes

After B.C. 407952 Standard Battery Heavy Duty Option (UA1) ----------------- ---------------- ----------------------- Battery 75-60 75A-60 Reserve Capacity 90 Minutes 90 Minutes Cold Cranking Amperage 500 Amperes 630 Amperes

Recommended service replacement batteries are Delco 75-60 (standard battery), or Delco 75A- 60 (heavy duty battery) or equivalent.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.