FUEL LINES FUEL INJ. ENGINES REPLACE WHEN NECESSARY. Cadillac Cimarron 1985

For 1990-2009 cars

# FUEL LINES FUEL INJ. ENGINES REPLACE WHEN NECESSARY

#### MODELS AFFECTED: 1985 2.8L CIMARRON

The fuel system used on the 1985 Cimarron V-6 Multi-port Fuel Injection (MFI) engine operates at a higher pressure than carbureted or throttle body injected engines.

Coupled hose assemblies are not to be repaired. If a hose is damaged, it must be replaced as an asse m bly.

Fuel boses requiring replacement should be ordered from GMWDD.

The 1985 Service Manual should be reviewed for specific fuel system pressure diagnosis and repairs.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.