MODEL PAINT INFORMATION LIST OF SUPPLIES/ORDERING CODE. Cadillac Commercial Limo/Hearse Chassis 1993

For 1990-2009 cars

# MODEL PAINT INFORMATION LIST OF SUPPLIES/ORDERING CODE

#### SUBJECT: 1993 MODEL PAINT INFORMATION

This bulletin is intended to provide a cross reference between factory paints and materials to the refinish products available in the field. It provides information about plastics identification and specific repairs required by some materials. It also provides a detailed list of the various suppliers' ordering codes for exterior, interior, vinyl roof moldings, and paint stripe colors. paint codes listed in the bulletin are, or some will be available from local paint suppliers.

Assembly Plant Paint Type Paint Supplier Paint Codes -------------- ----------------- ---------- --------- Hamtramck Clear Coat Enamel DuPont All Hamtramck (Allante) Clear Coat Enamel PPG All Orion Clear Coat Enamel PPG All Arlington Clear Coat Enamel DuPont All

Cadillac encourages the use of refinish materials that match the paint technologies and suppliers in our plants. However, other suppliers produce service paint which could perform satisfactorily for field repairs. Your local paint supplier can provide additional information.

The Service Parts Identification (SPID) label is located on the inside of the rear compartment area. This label contains the paint codes needed to identify the paint materials for field repairs. Note this label identifies the paint code along with the WA# for that paint code. It is equally important to use this WA# along with the paint code to identify the correct repair materials. Care should be taken to transfer the SPID label or its information if the panel to which the label is affixed requires replacement. Replacement SPID labels are not available

Depending on your body shop location, certain low VOC compliant materials may need to be substituted for the materials listed in this bulletin. Please check your local laws and regulations to determine the ability of the material to comply.

I. PLASTIC PARTS IDENTIFICATION

All 1993 Cadillacs have exterior parts made of various types of plastic materials that require specific Procedures to obtain high qualify refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1993 models. For best results when painting is required, determine the type of plastic material from the chart. Then follow the correct paint procedure, depending upon what painting material and equipment is available.

Plastic Type Symbol ------------------- ------------------ Thermoset Urethane RRIM (PU or PUR) Thermoplastic Urethane TPU Thermoset Polyester UP (SMC) Thermoset Urethane RIM (PU or PUR) Thermoplastic Elastomer TPE Thermoplastic Olefin TPO GTX 917 Nylon Xenoy PC, PBT Minlon PA

II. SPECIFIC REPAIR PROCEDURE

A. General Paint Procedure For Exterior Flexible Plastics

Polyvinylchloride (PVC); Polyurethane (PUR, TPUR, RRIM, RIM); Thermoplastic Elastomer (TPE); EPDM Rubber (supplied in prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to to the manufacturer's literature available through your jobber for details on proper mixing and application.

1. Thoroughly clean part by washing with a suitable cleaning solvent to remove all surface contaminates.

Cleaning Solvents: [low VOC alternate material shown in brackets]

a. DuPont 3919S Prep-Sol/Plastic Cleaner 2319S [3929 Prep-Sol or 3949S Cleaner]

b. BASF Pre-Kleano 900 [905 Water-Base Prep Cleaner]

c. PPG Acryli-Clean DX330 or DX103 Multi-Prep [DX380 Low VOC Cleaner]

d. Sherwin-Williams Kril-Kleen R1-K213 [Aqua-Mate W4K157]

e. Acme 6089; Rogers 4089 [Acme 87 Aqua-Klix, Rogers 4087, Kle-Car II]

f. Martin-Senour 6387 [6388 Kleanz Easy II]

#### IMPORTANT: Previously painted parts that show signs of cracking, peeling, or improper adhesion must be stripped before repainting.

2. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or finer) sandpaper and feather edge any damaged areas and rewash.

3. Apply two thin coats of primer, when required, per top coat manufacturer's recommendation and allow to completely dry before proceeding. (For most products, approximately 30 minutes.)

4. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes dry time between each double coat and allow to completely dry before using.

5. Following is a list of some of the products available for painting flexible plastic: [low VOC alternate material shown in brackets]

o PPG Flexible Primer - DPX844 [low VOC Plastic Primer DPW1844] o PPG Flexative - DX369 (Elastomeric Additive) or DC950 NCT o DuPont 9250S Flex Additive o Sherwin-Williams Multi-Flex - V6V299 o Acme/Rogers Multi-Flex - 68/4068 o Martin-Senour Flex Additive - 3084 o BASF Diamont Flex Agent DF-25; Glassodur Elastifier Additive 521-111 o R-M 891 Flex

B. Nylon - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts

C. Acrylonitrile-Butadiene-Styrene (ABS) - No prime required. Paint interior parts with acrylic lacquer.

D. Polyester Parts (UP, PBTP) - Will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

E. Polypropylene - Interior parts.

1. Wash surface thoroughly with cleaning solvent.

2. Apply primer immediately and allow to dry completely before color coating.

3. Color coat with lacquer or enamel reduced and applied according to the manufacturer's recommendation.

4. Materials: [Low VOC alternate material shown in brackets]

Cleaners: DuPont Prep-Sol 2319S DuPont 3939 Enamel Cleaner [3949 Metal Cleaner] DuPont 3812S Enamel Reducer PPG DX330 or DX103 [DX380 Low VOC Cleaner] Sherwin-Williams R1-K213 [Aqua-Mate W4K157] Acme 6089; Rogers 4089 [Acme 87 Aqua-Klix, Rogers 4087, Kle-Car II] Martin-Senour 6387 [6388 Kleanz Easy II]

Primer: DuPont 329S Polypropylene Primer GM 1052364 PPG DPX800 [DPW 1844 Plastic Primer] Sherwin-Williams P3C24 Acme/Rogers 524/4524 Martin-Senour 6242

F. GTX 917 Fender

1. The front fenders used on 1993 DeVilles and Fleetwoods are made of a rigid plastic nylon material known as GTX 917.

2. Procedures and materials for GTX 917 plastic fender are the same as those used on rigid SMC or sheet metal parts and do not require flex agent additives.

G. Xenoy

1. Allante front and rear bumpers and DeVille lower accent moldings are made of Xenoy materials. Xenoy parts will be supplied in colors. Use the same refinish procedures as on sheet metal parts for any required paint repairs.

H. Minlon

1. Center pillar hinge covers on the 1993 Seville are made of a rigid nylon material known as Minion.

2. Service parts will be supplied in prime, and refinish procedures should be the same as those used for sheet metal with no flex agents required.

III. BASE COAT REPLACEMENTS (BCR)

Base coat replacements, which are essentially color-keyed primers, are being utilized on 1993 DeVilles and Fleetwoods to improve the factory processing of the vehicles. Speci]Fic areas that will be painted with the BCR exposed include:

A. The Underside Of The Hood

B. The Motor Compartment

o Upper and lower radiator support o Front of dash panel o Shock towers

C. Back Side Of The Fuel Door

D. Rear Wheel Skirt Flange On The Fleetwood

Repairs to surfaces painted with BCR's should be done with base coat paint.

IV. REFINISH MATERIAL TABLES

The following tables provide specific field refinish materials for 1993 Cadillac colors.

1993 MODEL PAINT INFORMATION EXTERIOR

PAINT CODE COLOR NAME ------------------ SHERWIN MARTIN WILLIAMS AKZO/ WA# PPG DUPONT SENOUR ACME R.M. GLASURIT SIKKENS ----- ----- ------ ------ ------- ----- ------- --------- 04 Pearl Flax 9818 4550 B9256 46825 46825 22072 GM-9818 GMA92:04 4551 B9257 46826 46826

08 Mary Kay Pink Pearl (Allante) 9760 73255 K9379 45225 45225 GMA91:08 4178 K9380 45226 45226

08 Mary Kay Pink 9601 73365 K9340 45117 45117 20068 GM-9601 GMA88:08

09 Opaque White 9879 91013 B9167 45147 45147 21054 GM-9879 GMA91:09

13 Silver Metallic 9021 3822 D8590 90-6012 35369 15365 GM-9021 GMA85:13S

18 Dk Green Gray Metallic 9795 4453 B9211 47155 47155 21042 GM-9795 GMA92:18

22 Lt Sapphire Metallic 8966 3964 B8703 35879 35879 17003 GM-8966 GMA87:22

28 Blk Sapphire Metallic 8743 3885 B8618 90-6056 35313 16003 GM-8743 GMA86:28

33 Lt Driftwood Metallic 5322 4454 B9244 45754 45754 22269 GM-5322 GMA92:33

38 Champagne Metallic 9633 4263 B9004 42593 42593 20013 GM-9633 GMA90:38

40 White 8554 4318 B8469 90-5759 33755 13570 GM-8554 GMA84:40C

41 Black 8555 9700 99 90-5760 33756 13572 54-1240 GMA84:41C

41 Black (Allante) 9588 9729 99 39126 39126 18628 GM-9588 GMA91:41

47 Euro Red 9547 4126 D8891 38860 38860 18627 GM-9547 GMA88:47

55 Canyon Yellow 9814 4459 B9253 45735 45735 21046 GM-9814 GMA92:55

55 Euro White (Allante) 9868 4013 D8870 44389 44389 21047 GM-9868 GMA90:55 4014 D8722 44390 44390

57 Lt Beige Metallic 9805 4460 B9223 45736 45736 21045 GM-9805 GMA92:57

58 Canyon Yellow Pearl 5397 4705 B9215 46806 46806 23012 GM-5397 GMA92:58 4706 B9216 46807 46807

59 Bronze Metallic 9894 4707 B9318 46832 46832 23018 GM-9894 GMA93:59

63 Med Taupe Metallic 9811 4462 B9245 45750 45750 22260 GM-9811 GMA92:63

72 Med. Garnet Red Metallic 8979 3986 B8713 35894 35894 17021 GM-8979 GMA87:72

77 Dark Cherry Metallic 9800 4465 B9210 45739 45739 22261 GM-9800 GMA92:77

81 Bright Red 8T74 3794 C8508 90-5954 34983 15265 GM-8774 GMA85:81

83 Med. Sapph Blue Metallic 8993 3995 B8720 35900 35900 17028 GM-8993 GMA87:83

84 Pearl Red 9976 4553 B9260 46827 46827 22075 GM-9976 GMA92:84C 4554 B9261

87 Gun Metal Metallic 5328 4009 B9252 46040 46040 22270 GM-5328 GMA92:87

88 Dark Plum Metallic 9813 4467 B9220 45741 45741 22262 GM-9813 GMA92:88

91 Polo Green Metallic 9529 4235 D8871 42595 42595 18038 GM-9529 GMA90:91

93 White Diamond 8933 4175 B8609 39244 39244 16021 GM-8933 GMA89:93 3680 B8469 39245 39245

1993 MODEL PAINT INFORMATION INTERIOR COLORS

PAINT CODE COLOR NAME --------------------- WA# PPG DUPONT MARTIN-SENOUR SHERWIN-WILLIAMS ACME BASF 5deg 12deg 5deg 12deg 5deg 12deg 5deg 12deg --- ---- ------- ------------ ------------ ------------ --------- 11 White 3835 90232 C8538 17172 17029 35574 33777 35574 33777 11526 4402

14 Light Gray 9781 35382 C9222 46228 46229 46228 46229 46228 46229 22296 22286

14 Medium Gray 9779 35386 C9220 46230 46231 46230 46231 46230 46231 22297 22284

14 Dark Gray 9902 35387 C9223 46232 46233 46232 46233 46232 46233 22298 22273

17 Charcoal 9545 9777 C9224 46234 46234 46234 33024 22227 22226

19 Black 848 9640 C8535 16615 16918 J4-8677 33024 92387 33024 12812 4401

20 Very Dark Sapphire 8841 16202 C8770 36571 36479 36571 36479 36571 36479 17095 17094

38 Light Natural Beige 9606 26728 C9225 46236 46236 46236 21114 21113

38 Dark Natural Beige 9581 27102 C9254 46238 46238 46238 22231 22230

52 Light Neutral 9772 27303 C9226 46240 46241 46240 46241 46240 46241 22232 22283

52 Med. Dark Neutral 9648 27305 C9228 46242 46243 46242 46243 46242 46243 22234 22272

54 Taupe 9775 27306 C9229 46244 46245 46244 46245 46244 46245 22235 22294

63 Light Saddle 5330 27308 C9306 47661 47670 47661 47670 47661 47670 23038 23039

63 Medium Saddle 9777 27308 C9231 45944 45945 45944 45945 45944 45945 22277 22278

63 Dark Saddle 9778 27309 C9232 45946 45947 45946 45947 45946 45947 22279 22280

66 Medium Beechwood 9098 26250 C8805 38601 38218 38601 38218 38601 38218 18046 18047

66 Dark Sienna 8856 25916 C8811 38220 38382 38220 38382 38220 38382 18045 17104

71 Medium Maroon 9064 51370 C9233 46246 46246 46246 21108 21107

71 Dark Maroon 9063 51371 46248 46248 46248 21106 21105

75 Bordeaux Red 9934 51770 C9308 47253 47668 47253 47668 47253 47668 22242

78 Garnet Red 8781 72799 C8616 17134 35433 35433 17085 16055

1993 MODEL PAINT INFORMATION VINYL COLORS

PAINT CODE COLOR NAME ----------------- MARTIN SHERWIN WA# PPG DUPONT SENOUR WILLIAMS ACME BASF ---- ------ ------ ------ -------- ---- ----- 13T Bright Silver Metallic 7781 2-1052 B8402 26704 34123 34123 14039

18T Dark Green Gray 9795 2-1449 B9211 46220 46220 46220 22221

22T U. Sapphire Blue Metallic 8966 2-1271 B8703 36595 36595 36595 17066

26T Dark Blue 8712 2-891

26T Dark Blue 8841 C8770

28T Black Sapphire Metallic 9994 2-1273 46226 46226 46226 17068

33T Light Driftwood Metallic 5322 2-1450 B9244 46678 46678 46678 22243

40T White 3967 2-917 5338 47860 47860 47860 16110

40T White 8936 2-130 B8469 26851 35781 35781 16110

41T Black 8 48 2-120 B8479 15518 J4-1990 9739 4416

57T Light Beige Metallic 9805 2-1453 B9223 46227 46227 46227 22244

59T Bronze Metallic 9894 2-1516 B9318 47787 47787 47787 23035

63T Medium Taupe Metallic 9811 2-1454 B9245 46223 46223 46223 22245

72T Garnet Red Metallic 8979 2-1268 B8713 36596 36596 36596 17073

76T Dark Garnet 9344 2-1272

77T Dark Cherry Red Metallic 9800 2-1456 B9210 46224 46224 46224 22224

83T Medium Sapphire Blue 8993 2-1274 B8720 36600 36600 36600 17074

87T Gun Metal Metallic 7782 2-1053 B8403 26705 34124 34124 14040

88T Dark Plum Metallic 9813 2-1457 B9220 46225 46225 46225 22225

1993 MODEL PAINT INFORMATION PAINT STRUPE COLORS

PAINT CODE COLOR NAME ------------------ MARTIN SHERWIN AKZO/ WA# PPG DUPONT SENOUR WILLIAMS ACME BASF SIKKENS --- ------ ------ ------- -------- ----- ----- -------- 14A Light Gray 8670 33856 C85929 26729 34869 34869 15165 GMA90:14A

21A Dark Sapphire Blue 9103 16313 C8787 36464 36464 36464 17055 GMA90:21A

22A Light Sapphire Blue 7456 15474 D8009 26459 31420 31420 12370 GMA91:22A

40A White 3967 2058 5338 32-3929 J4-2588 5644 2080 GMA91:40A

41A Black 848 9300 99 8803 01738 83 PKG GMA91:41A

48A Sandstone 7260 3327 B8105 46101 46101 46101 22218 GMA92:48A

54A Gold 9836 27063 C9061 43819 43819 43819 20029 GMA90:54A

57A Dark Teal 5340 18340 C9260 46525 46525 46525 23030 GMA92:57A

62A Light Taupe 5301 51687 C9252 46102 46102 46102 22217 GMA92:62A

66A Dark Auburn 9646 26796 C9038 43372 43372 43372 20033 GMA91:66A

75A Red 4721 72128 43592 26272 J4-7191 11892 4518 GMA90:75A

79A Dark Claret 8663 51167 C8525 26728 34868 34868 15071 GMA90:79A

87A Dark Gray 8291 3375D C8441 26700 34102 34102 14036 GMA91:87A

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.