GAP INNER DOOR PANEL & DOOR TRIM (REAR DOOR). Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# GAP INNER DOOR PANEL & DOOR TRIM (REAR DOOR)

#### SUBJECT: GAP BETWEEN INNER DOOR PANEL AND DOOR TRIM ON REAR DOOR (REPLACE REAR UPPERMOST DOOR TRIM FASTENER)

#### VEHICLES AFFECTED: 1991 "C" MODELS

Some 1991 Fleetwood vehicles may exhibit a condition where a gap between the inner door panel and the door trim on either rear door is noted. The gap is at the rear of the door trim pad at the belt line area.

To correct this condition, replace the existing rear uppermost door trim fastener with part number 10121502.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.