REAR WINDOW LACE PAINT REPAIR (SERVICE PROCEDURES). Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# REAR WINDOW LACE PAINT REPAIR (SERVICE PROCEDURES)

#### SUBJECT: REAR WINDOW LACE PAINT REPAIR

#### VEHICLES AFFECTED: 1989-1992 "C" DEVILLES, FLEETWOODS AND 60 SPECIAL

This bulletin contains rear window lace paint repair information for 1989-92 DeVilles, Fleetwoods and 60 Specials without vinyl roofs. The following paint systems from PPG, DuPont and RM are intended for spot repairs or the entire primed lace as supplied by CANSPO. They should be applied with the lace installed on the car with adjacent surfaces suitably protected.

The following recommendation is for Deltron acrylic urethane base coat with NCT flexible clear coat.

#### PPG

1. Solvent wipe substrate with DX-330 Grease and Wax Remover using clean, lint-free towels.

2. Apply one medium coat of DSX-1900 Bonding Clear. Allow 5-10 minutes flash time.

3. Base coat reduction - 1 part colour: 1-1/2 - 2 parts DRR reducer.

#### IMPORTANT: Use appropriate reducer for shop conditions.

APPLICATION: Apply 2-3 medium coats of base coat. Allow 5-10 minutes between coats. Let base coat dry for 15 minutes before applying clear.

4. NCT clear coat reduction - 1 part clear: 1 part activator: 1/4 part flex agent.

#### IMPORTANT: Use appropriate activator for shop conditions.

APPLICATION: Apply two wet coats of clear. Allow 5-10 minutes between coats.

#### IMPORTANT: If dry edge appears, blend immediately with one coat of DT-95 solvent.

Allow overnight air dry or force dry at 180 F for 30 minutes before putting into service.

#### Materials Required

DBU Factory Package Colour DRR Reducer (1170, 1185) DX-1798 Flex Agent DC Activator (1260,1275,1290) DT-95 Solvent (for blending) DX-330 Grease and Wax Remover DSX-1900 Bonding Clear

DUPONT

#### Centari Acrylic Urethane Enamel:

1. Solvent wipe surface with 3939S Lacquer and Enamel Cleaner. 2. Apply Centari Basemaker to full hiding per label directions. 3. Upon proper dry, apply two coats of 1080S Uro Clear per label directions.

#### Cronar Polyoxithane Enamel

1. Solvent wipe surface with 3939S Lacquer and Enamel Cleaner. 2. Apply one coat of 9222S Cronar Adhesion Promoter. 3. Apply Cronar Polyoxithane Enamel base coat per label directions. 4. Upon proper dry, apply two coats of 1080S Uro Clear per label directions.

#### RM

The following recommendation is for Diamond base coat/clear coat for Cadillac/flexible rubber moulding.

1. Solvent wipe the flexible rubber moulding with 900 Pre-Kleano Wax and Silicone Remover using lint-free cloth.

2. Light scuff OEM painted substrate with Scotchbrite-Ultra fine grade, then solvent rinse with 901 Pre-Paint Cleaner.

3. Apply one medium wet coat of Diamont base coat colour or until hiding has been achieved. Allow 3-5 minutes flash in between coats.

REDUCTION - Base coat colour - 2 parts by volume BR Reducer - 2 parts by volume

#### IMPORTANT: Use appropriate reducer for Shop condition. Allow at least 15 minutes to flash before applying flexible clear coat.

4. DC-88 Flexible clear coat reduction - DC-88 Diamond Clear: 4 vol. parts DH-44 Hardener: 1 vol. parts

Application: Apply two wet coats of above clear. Allow 5-10 minutes flash time in between coats.

5. Overnight drying at room temperature is suggested but could be force dried at 38 C (160 F) for at least 60 minutes before putting into service.

#### Material Requirements:

Diamond Base Coat Colours Diamond DC-88 Clear BR-50/BR-60 Base Coat Reducers Diamond DH-44 Hardener Pre-Kleano 900 Wax/Silicone Remover 901 Pre-Paint Cleaner

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.