LABOR TIME GUIDE REQUEST FOR REVIEW UPDATE. Cadillac Commercial Limo/Hearse Chassis 1991

For 1990-2009 cars

# LABOR TIME GUIDE REQUEST FOR REVIEW UPDATE

#### SUBJECT: LABOR TIME GUIDE REQUEST FOR REVIEW UPDATE

This bulletin contains information on Labor Time Guide Requests For Review received between January 1, 1991 and March 15, 1991. We have received 62 requests, with 53 resulting in increased time allowances or new operations. These changes will appear in the 1991 LTG revision and are summarized on the attached sheets. Time increases are indicated as +, time decreases as -, no change as NC, and new operations as NOP.

Thank you to all dealers who have submitted Requests For Review; we appreciate your input. Request For Review forms are provided at the back of your Labor Time Guide. If you have any questions or concerns, please submit a Request For Review form or call Ann Haener-Maghran at (313) 554-6946.

LABOR | DESCRIPTION |YEARS | C | D | E | K | V OPERATION| | | | | | | ---------|----------------------------------|-------|---|---|---|---|--- B0550/51 |Filler,Lower Headlamp Opening - | 1991 | .2| | | | NOP | Replace | | .5| | | | | ADD: to refinish | | AE| | | | | ADD: to color coat | | .4| | | | | | | AD| | | | B3557 |Backlite Straps, Adjust |1987-91| | | | | .2 NOP | INC: Both straps | | | | | | | | | | | | | B6005 |Hinge, Fuel filler door - Replace |1987-91| | | | | .5 NOP |ADD: to color/clear coat | | | | | | .1 | | | | | | | GA | | | | | | | B8648 |Molding and/or Applique,Rear | | | | | | | Compartment Lid outer Panel - | | | | | | | R&R or Replace | 1991 | .2| | | | NOP | | | | | | | C0140/41 |Channel,Front Door Window Run - | | | | | | | R&R or Replace |1990-91| .6| | | | - | | | | | | | C2540 |Panel Carrier Assmy., Instrument | | | | | | | Control - Replace |1990-91| | |2.9|2.9| + | | | | | | | C6430/31 |Cable,Front Seat Rear Vertical | | | | | | | Drive - R&R or Replace |1990-91| | .8| | | + | | | | | | | C6516/17 |Actuator, Front Seat Back (Power |1990-91| | | | | | Reclining or Release Unit) Split/| | | | | | | Divided-R&R or Replace | | | .8| | | NOP | | | | | | | C9040/41 |Belt,Safety Front (Retractor Side)| | | | | | | R&R or Replace |1987-88| | | | | + | |"J" at | | | | | | | .6 | | | | | | | | | | | | C9200 |Belt, Safety Rear (Retractor Side)| | | | | | | Replace |1989 | .6| | | | + | | | | | | | D0362 |A/C Control Assmy - Replace |1991 | .5| | | | + | | | | | | | D0540 |Sensor,In-Car - Replace |1991 | | | .5| .5| + | | | | | | | D1113 |Switch, Compressor Cut-Off - Power| | | | | | | Steering - Replace |1991 | .4| | | | + | | | | | | | D2782 |Hoses,Heater (With Air Condition- | | | | | | | ing) Cylinder Block To Head To | | | | | | | Core - Replace |1986-88| | | .7| .7| + | | | | | | |

=============================================================================

LABOR | DESCRIPTION |YEARS | C | D | E | K | V OPERATION| | | | | | | ---------|----------------------------------|-------|---|---|---|---|--- D2828 |Core, Heater - Replace |1990-91|1.0| |1.4|1.4| + | | | | | | | D3088 |Hoses and/or Lines, Refrigerant - | | | | | | | Compressor Suction and Discharge| | | | | | | Hose Assembly |1990-91| | | | | .7 + |ADD: recover/recharge A/C system | | | | | | .7 | | | | | | | D4300 |Seal,Seat, and/or O-Ring, | | | | | | | Compressor Shaft - Replace R4 |1990-91| | .6| | | NOP |ADD:recover/recharge A/C system | | | .7| | | | HR6 | 1991| .9| |1.3|1.3|1.6 NOP |ADD:recover/recharge A/C system | | .7| | .7| .7| .7 | | | | | | | | | | | | | | E0200 |Wheel, Balance - One | 1990| | .3| | | NC E0201 |Wheel, Balance - Two | | | .5| | | NC E0203 |Wheel, Balance - Four | | | .7| | | NC | | | | | | | E3920/21 |Mount Assembly, Front Strut | | | | | | | Bearing - Replace | 1991| .9| | | | + | | | | | | | E3927 |Mount Assembly, Front Strut | | | | | | | Bearing - Replace (Both) | 1991|1.6| | | | + 7200 |Cylinder, Ignition Lock - R&R or | 1989| | |1.4| | NC | Replace | | | | | | E7200 |Cylinder, Ignition Lock-R&R |1990-91| | |1.0|1.0| | or Replace | | | | | | E7301/02 |Housing, Steering Shaft | | | | | | | Bearing-R&R or Replace |1986-91| | |2.3|2.3|2.3 NC |ADD: to color coat | | | | .3| .3| .3 + | | | | |GB | GB| GB | | | | | | | E7501 |Locking Parts,Rack/Selector/ | | | | | | | Lock Bolt/Actuator Rod, Steer- | | | | | | | ing Column - Replace |1990-91|1.6| | | | + | | | | | | | E9050 |Pump Assembly, Power Steering - | | | | | | | Replace |1990-91| .9| | | | + | | | | | | | H01 27 |Disc Assembly, Front Both - | | | | | | | R&R or Replace | 1990| |1.2| | | NC | | | | | | | H2505 |Module, Electronic Brake | | | | | | | Control (ABS) - Replace | 1991| .5| .3| | | .4 NOP

============================================================================

LABOR OPERATION| DESCRIPTION | YEARS | C | D | E | K | V --------------------------------------------------------------------------- J0200 |Manifold and/or Gasket, Intake - |1990-91| | |4.6|4.6| + | Replace | | | | | | J0520 |Valve, Recondition or Replace |1990-91| | | | | | | | | | | | |ADD: to recondition all valves | | | | | | | | | | | | | |INC: replace valves as necessary | | | | | | | Right | | | .9| | | + | Left | | | .9| | | + | Both | | |1.7| | | + J0955 |Tube and/or Seal, Oil | | | | | | |Distribution - Replace |1991 | .8| | | | - | | | | | | | J1000 |Pan and/or Gasket, Oil - Replace |1986-90| | |1.4|1.4| + | | | | | | | J1020 |Pump, Engine Oil - Replace |1990-91| |1.9| | | + |ADD: to recondition oil pump | | | .2| | | | | | | | | | J1150 |Bearing, Crankshaft Main - Replace| 1987| | |1.8| | NC | | | | | | | J4437 |Sensor, Electronic Spark Control | | | | | | | Knock - Replace | 1991| | .3| | | NC | | | | | | | J6134 |Pipe, AIR - Check Valve to Left | | | | | | |Exhaust Manifold |1988-89|1.7| |1.7|1.7| + | | | | | | | J6358 |Motor, Idle Speed Control - Adjust| 1991| | | .6| .6| NC | | | | | | | J6374 |Sensor, Throttle Position - | 1991| .8| | | | + | Replace | | | | | | J6383 |Switch, Neutral/Park - Replace |1990-91|1.1| | | | + | | | | | | | K6310 |Sensor, Transaxle Speed - Replace |1990-91| | .3| | | - | | | | | | | L2420 |Pipe, Intermediate Exhaust - |1986-91| | |1.1|1.1| + | Replace |1987-91| | | | |1.1 + | | | | | | | N0110 |Battery - Replace |1990-91| .5| | .5| .5| .5 + N0120 |Cables, Battery to Starter - |1989-91| .8| | | | + | Replace | | | | | | N1287 |Lens and/or Gasket, Lamp-All - |1990-91| | | | .4| + | Replace | | | | | | N2133 |Switch, Door Lock Remote Control -| | | | | | |Replace | 1991| .2| | | | NOP N2135 |Switch, Door Window Lockout | 1991| .3| | | | NOP N2610 |Switch, Windshield Wiper - | | | | | | |Replace (With Tilt) |1990-91|1.5| | | | + N2620 |Switch, Windshield Wiper Motor | 1990| .7| .6| .7| .7| NC | Park | | | | | |

============================================================================

LABOR | DESCRIPTION | YEARS | C | D | E | K | V OPERATION| | | | | | | ---------------------------------------------------------------------------- N2910 |Relay, Theft Deterrent |1990-91| .4| | | | + | Interrupt - Replace | | | | | | N3324/25|Motor, Door Window - Rear - |1989-91| .9| | | | + | Replace | | | | | | N3460 |Motor, Brake Transmission Shift | | | | | | | Interlock - Replace | 1991 | .7| | | | NOP | | | | | | | N3475 |Brake Transmission Shift | 1991 | .6| | | | NOP | Interlock, Adjust | | | | | | N3570 |Module, Pulse Wiper Control - |1990-91| .5| | | | + | Replace | | | | | | N4180 |Instrument Panel Cluster Assembly | | | | | | |(Digital/Electromechanical) - R&R | | | | | | | or Replace (Replaces Labor |1990-91| .6| .3| .4| .4| .4 NC | Op N4300) | | | | | | N5140 |Instrument Cluster Circuit, | | | | | | |Printed -R&R or Replace |1990-91| .9| | | | + | | | | | | | N6580 |Wiring and/or Connector - | | | | | | | Windshield Wiper Motor/Washer |1990-91| .5| | | | NOP | Pump - Repair | | | | | | | | | | | | | R0440 |Antenna Components-Power Lead In- | | | | | | |Replace Both Pieces |1986-91| | |1.0|1.0| + | | | | | | | R2972 |Theft Deterrent System Components | | | | | | |Components - Key (VATS) - Replace |1990-91| .2| | .2| .2| .2 NOP | | | | | | | R2975 |Theft Deterrent System Components | | | | | | |Components Module (VATS) - Replace|1990-91| .7| | | | + | | | | | | | R4045 |Switch, Rear Compartment Lid | | | | | | |Closing Unit - Replace |1990-91| | | | | .4 + | | | | | | | R9000 |Vehicle Security and Keyless Entry| | | | | | |System Components - Base System - | | | | | | |Replace |1989 | .5| | .5| .5| .5 NC | |1990-91| .5| .5| .5| .5| .5 NC | | | | | | | T6276 | Seal Pack - Bulletin T-88-59 |1987-88| | | | | .2 NOP |

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.