4th Band Installation. Cadillac Concours 1997

For 1990-2009 cars

#### Tools Required

J 34741-3 Input Shaft Seal Sizer

1. Install the fourth band (523) into the case. Seat the band properly onto the anchor pin with the seat of the servo pin toward the servo bore in the case.

Important: Leave the J 34741-3 in place until the reverse clutch and housing assembly is ready to be installed.

2. Install the J 34741-3 over the input shaft oil seal rings. Use a twisting motion to install the J 34741-3 . The J 34741-3 must contact the third clutch housing hub.