DTC P0133 HO2S Slow Response Bank 1 Sensor 1. Cadillac Concours 1996

For 1990-2009 cars
Engine Controls Components
Heated Oxygen Sensors
OBD II Symbol Description Notice
ESD Notice

### Circuit Description

The PCM provides a 0.45 volt reference signal to the oxygen sensor on CKT 1666. When the oxygen sensor is cold, below 200°C (392°F), the oxygen sensor signal voltage will be around 0.45 volt and the PCM will keep the system in Open Loop operation. When the oxygen sensor is warm, above 200°C (392°F), the oxygen sensor will swing from rich to lean rapidly, if the PCM is in good control of the air fuel mixture. DTC P0133 is designed so that if the oxygen sensor is slow to respond to changes in exhaust oxygen content, this DTC will set.

### Conditions for Setting the DTC

#### Test Conditions

• | DTCs P0117, P0118, P0121, P0122, P0123, P0135 and P1133 not set.

• | This test has not been completed yet this ignition cycle.

• | Low coolant level not present.

• | Ignition voltage between 9 volts and 16 volts.

#### Failure Conditions

• | Average time to change from rich to lean greater than 0.15 seconds.

• | Average time to change from lean to rich greater than 0.15 seconds.

### Action Taken When the DTC Sets

• | The PCM will illuminate the Malfunction Indicator Lamp (MIL) after two consecutive drive trips that the diagnostic runs and fails.

• | The PCM will record operating conditions at the time the DTC sets. This information will be stored in the Freeze Frame and Failure Records.

• | A first failure of this DTC will store in Last Test Failed but not History.

### Conditions for Clearing the MIL/DTC

• | The PCM will turn the MIL OFF after three consecutive drive trips that the diagnostic runs and does not fail.

• | A Last Test Failed DTC will clear when the diagnostic runs and does not fail.

• | A History DTC will clear after forty consecutive warm-up cycles with no failures of any diagnostic test.

• | Use a scan tool to clear DTCs.

• | Interrupting PCM battery voltage may or may not clear DTCs. This practice is not recommended. Refer to Clearing Diagnostic Trouble Codes in PCM Description and Operation.

### Diagnostic Aids

Notice: Do not solder heated oxygen sensor wires. Soldering the wires will result in the loss of the air reference to the sensor. Refer to Engine Electrical for proper wire and connection repair techniques.

### Test Description

Number(s) below refer to the step number(s) on the Diagnostic Table.

1. Checking if other possible causes of this DTC have already been diagnosed.

2. Diagnose other DTCs first because they may be the cause of this DTC setting.

3. With the engine running warm, coolant at least 85°C (185°F) and at fast idle, the oxygen sensor voltage should rapidly swing above 0.60 volt and below 0.30 volt.

4. The loop status on the scan tool will change from Open Loop to Closed Loop when the PCM enters fuel control. Under these conditions, the PCM should be in Closed Loop.

5. Checking if the oxygen sensor voltage is swinging between rich and lean very slowly, or not at all.

6. Checking for causes of oxygen sensor failure. If sensor is replaced without finding cause of contamination, contamination of new sensor may result.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to A Powertrain On Board Diagnostic (OBD) System Check
2 | Were you sent here from another DTC? | -- | Go to Step 4 | Go to Step 3
3 | Are any other PCM DTCs set? | -- | Diagnose other PCM DTCs first | Go to Step 4

4

1. Connect a scan tool, start engine.
2. Start engine, warm-up until engine coolant temperature is the same or more than the value specified.
3. View the Bnk. 1 Sns. 1 oxygen sensor voltage display.
4. Operate engine at steady 1200-2000 RPM for 2 minutes.

After 2 minutes does the rear oxygen sensor voltage rapidly swing outside the range specified?

85°C (185°F)

0.3 - 0.6 volts

Go to Step 5

Go to Step 6

5 | With engine running at 1200-2000 RPM, view Loop Status on the scan tool. Does the loop status indicate Closed? | -- | Go to Step 10 | Go to Step 9
6 | Does the rear oxygen sensor voltage remain between the voltage range specified longer than the time it swings outside the range specified? | 0.3 - 0.6 volts | Go to Step 9 | Go to Step 7

7

1. Check terminal contact at PCM connector C2 terminals 65 and 66.
2. Repair terminal contact if needed.

Was terminal contact repaired?

--

Go to Powertrain Control Module Diagnosis for Verify Repair

Go to Step 8

8

1. Check terminal contact at the rear oxygen sensor connector.
2. Repair terminal contact if needed.

Was terminal contact repaired?

--

Go to Powertrain Control Module Diagnosis for Verify Repair

Go to Step 9

9

1. Replace rear oxygen sensor. Refer to Heated Oxygen Sensor (HO2S) Replacement (Rear) .
2. Check for possible causes of oxygen sensor contamination:

• | Leaded fuel.

• | Incorrect gasket sealer.

• | Over rich operation.

Were any of these possible causes found?

--

Take necessary corrective action

Refer to Fuel System Check

10 | Check for possible causes of extended rich or lean operation Were possible causes noted and repaired? | -- | Go to Powertrain Control Module Diagnosis for Verify Repair | System OK