Air Filter Element and Air Cleaner Assembly. Cadillac Concours 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the intake air duct from the mass air flow sensor.
2. Lift the air cleaner element assembly (1) off of the air inlet assembly (2) locating pins.
3. Slide the air cleaner element assembly (1) toward the fender to unseat the locating tab of the air cleaner element assembly (1) from the slot of the air inlet assembly (2).
4. Remove or disconnect the Intake Air Temperature sensor.
5. Remove the air cleaner element.
6. Remove the air cleaner element assembly (1).

### Installation Procedure

1. Install the air cleaner element.
2. Ensure the rubber locating grommets are secure in the bottom of the air cleaner element assembly (1).
3. Slide locating tab on bottom of the air cleaner element assembly (1) down into the slot on the top of air inlet assembly (2).
4. Press the air cleaner element assembly (1) down onto the locating pins ensuring the locating grommets are secure in the bottom of the air cleaner element assembly (1).
5. Install or connect the Intake Air Temperature sensor.
6. Install the intake air duct to the mass air flow sensor.

Tighten
Tighten the clamp assembly to 3.5 N·m 31 lb in.