Fastener Tightening Specifications. Cadillac Concours 1997

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accumulator Housing Cover Bolt | 8-14 N·m | 6-10 lb ft
Accumulator Housing to Channel Plate Bolt | 8-14 N·m | 6-10 lb ft
Bottom Pan to Case Bolt | 10-12 N·m | 8-9 lb ft
Case Cover to Case Bolt (10 mm) | 20-27 N·m | 15-20 lb ft
Case Cover to Case Bolt (13 mm) | 27-31 N·m | 20-23 lb ft
Case Cover to Case Stud (10 mm) | 20-27 N·m | 15-20 lb ft
Case Cover to Case Stud (13 mm)(47) | 27-31 N·m | 20-23 lb ft
Case Cover to Driven Sprocket Support Bolt | 20-27 N·m | 15-20 lb ft
Case Extension to Case Bolt (10 mm) | 20-27 N·m | 15-20 lb ft
Case Extension to Case Bolt (13 mm) | 50-55 N·m | 37-40 lb ft
Case Extension to Case Stud | 50-55 N·m | 37-40 lb ft
Case to Forward Clutch Support Stud | 25-27 N·m | 19-20 lb ft
Channel Plate to Accumulator Housing Bolt | 8-14 N·m | 6-10 lb ft
Channel Plate to Case Bolt | 8-14 N·m | 6-10 lb ft
Channel Plate to Case Nut | 8-14 N·m | 6-10 lb ft
Cooler Connector to Cooler (Case Cover) | 20-27 N·m | 15-20 lb ft
Detent Lever and Roller Assembly Bolt | 8-14 N·m | 6-10 lb ft
Differential to Final Drive Carrier Bolt | 70-76 N·m | 52-56 lb ft
Drive Sprocket Support to Case Bolt | 11-13 N·m | 8-9.5 lb ft
Input Speed Sensor to Case Bolt | 11-13 N·m | 8-9.5 lb ft
LCVB to Channel Plate Bolt | 8-14 N·m | 6-10 lb ft
Manual Shaft to Detent Lever Nut | 27-34 N·m | 20-25 lb ft
Oil Drain-Bottom Pan to Case Cover Plug | 8-14 N·m | 6-10 lb ft
Oil Test - #40 TORX® (Case Cover) Plug | 18-26 N·m | 13.5-19 lb ft
Oil Transfer Plate to Case Bolt | 8-14 N·m | 6-10 lb ft
Pressure Control Solenoid Bracket to UCVB Bolt | 11-13 N·m | 8-9.5 lb ft
Pump Assembly to Case Bolt | 11-13 N·m | 8-9.5 lb ft
Pump Assembly to Case Cover Bolt | 11-13 N·m | 8-9.5 lb ft
Return (Case) Cooler Connector | 25-29 N·m | 19-21 lb ft
Scavenge Pump Cover to Scavenge Pump Body Bolt | 11-13 N·m | 8-9.5 lb ft
Scavenge Tube to Case Bolt | 8-14 N·m | 6-10 lb ft
Secondary Pump to Case Bolt | 11-13 N·m | 8-9.5 lb ft
Secondary Pump to Case Cover Bolt | 11-13 N·m | 8-9.5 lb ft
Servo Cover to Case Bolt | 8-14 N·m | 6-10 lb ft
Side Cover to Case Cover Bolt (13 mm) | 20-27 N·m | 15-20 lb ft
Side Cover to Case Cover Bolt (15 mm) | 50-55 N·m | 37-40 lb ft
Side Cover to Case Cover Stud | 50-55 N·m | 37-40 lb ft
Spacer Plate Support to Channel Plate Bolt | 8-14 N·m | 6-10 lb ft
Speed Sensor to Case Extension Bolt | 8-14 N·m | 6-10 lb ft
Temperature Sensor | 3.4 N·m | 30 lb in
UCVB to Case Bolt | 11-13 N·m | 8-9.5 lb ft
UCVB to Case Cover Bolt | 11-13 N·m | 8-9.5 lb ft
UCVB to Driven Sprocket Support Bolt | 11-13 N·m | 8-9.5 lb ft