INFO - USE OF LOCTITE (R) ON FRONT LOWER CONTROL. Cadillac Concours 1997

For 1990-2009 cars

# INFO - USE OF LOCTITE (R) ON FRONT LOWER CONTROL

#### SUBJECT: INFORMATION - USE OF LOCTITE(R) ON FRONT LOWER CONTROL ARM TO BALL JOINT

#### MODELS: 1997 CADILLAC DEVILLE WITH B9Q, V4U

BUILT BETWEEN THE FOLLOWING VIN BREAKPOINTS:

OPTION B9Q: VU500000 - VU500198 OPTION V4U: VU700000 - VU700182

WHEN SERVICING VEHICLES BUILT WITHIN THE ABOVE LISTED VIN BREAKPOINTS, A CONDITION MAY OCCUR, WHEREBY IF LIFTED BY THE LOWER CONTROL ARM, THE BALL JOINT MAY SEPARATE FROM THE LOWER CONTROL ARM. IF THESE VEHICLES ARE TO BE LIFTED BY THE LOWER CONTROL ARM, OR IF THE BALL JOINT BECOMES SEPARATED, PERFORM THE FOLLOWING PROCEDURE.

#### PROCEDURE:

APPLY A COATING OF LOCTITE RC/609, OR EQUIVALENT, TO THE PERIMETER OF THE BALL JOINT SURFACE WHERE IT IS PRESSED INTO THE FRONT CONTROL ARM BY FOLLOWING THE STEPS BELOW.

1. RAISE AND SUPPORT THE VEHICLE.

2. CLEAN THE TOP SURFACE OF THE FRONT LOWER CONTROL ARM AROUND THE LOWER BALL JOINT HOUSING USING LOCTITE(R) PRIMER T747, OR EQUIVALENT. APPLY ENOUGH PRIMER TO ENSURE THAT IT WILL FLOW BETWEEN THE BALL JOINT HOUSING AND THE LOWER CONTROL ARM. DO NOT ALLOW THE PRIMER TO COME IN CONTACT WITH THE LOWER BALL JOINT SEAL. ALLOW THE PRIMER TO DRY 15 MINUTES.

3. APPLY A BEAD, APPROXIMATELY 3 MM (1/8 IN.) WIDE OF LOCTITE RC/609, OR EQUIVALENT, AROUND THE COMPLETE PERIPHERY OF THE BALL JOINT HOUSING AND LOWER CONTROL ARM INTERFACE (TOP SURFACE OF LOWER CONTROL ARM). ENSURE THAT THE BEAD OF LOCTITE(R) RC/609, OR EQUIVALENT, IS CONTACTING THE BALL JOINT HOUSING AND THE CONTROL ARM (SEE FIGURE 1).

4. WITH A BRASS HAMMER, STRIKE THE BOTTOM OF THE LOWER CONTROL ARM REPEATEDLY AROUND THE BALL JOINT. THIS WILL ENCOURAGE PENETRATION OF THE LOCTITE(R), OR EQUIVALENT, BETWEEN THE BALL JOINT HOUSING AND THE LOWER CONTROL ARM. DO NOT WIPE OFF EXCESS LOCTITE(R) RC/609, OR EQUIVALENT.

5. ALLOW THE LOCTITE(R), OR EQUIVALENT, TO CURE PER THE PACKAGE DIRECTIONS. ANY EXCESS LOCTITE(R), OR EQUIVALENT, MAY BE WIPED OFF AT THIS TIME.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T2282 LABOR OPERATION TIME: 0.3 HR

FIGURES: 01 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.