Starting and Charging Components. Cadillac Concours 1996

For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Battery | RH front corner of Engine Compartment | -- | 6D1-1 | --
Engine Compartment Fuse Block/Relay Center | Forward of LH front strut Tower | 8A-201-7 Fig. 15 | 11-0, 19-4 | --
Generator | Lower RH front of engine | 8A-201-15 Fig. 30 | 6D3-1 | --
Ignition Switch | Behind LH side of I/P, on Steering Column | 8A-201-30 Fig. 57 | 3F-1 | --
Instrument Panel Cluster (IPC) | LH side of I/P | 8A-201-26 Fig. 51 | 8C1-1 | --
LH Maxi® Fuse Block | Forward of LH front strut tower, near Engine Compartment Fuse/Relay Center | 8A-201-7 Fig. 15 | 10-0 | --
Park/Neutral Position Switch | On LH of Transmission, near base of rear Engine Lift Hook | 8A-201-20 Fig. 39 | 202-37 | --
Powertrain Control Module (PCM) | LH front corner of Engine Compartment, under Air Cleaner Housing | 8A-201-4 Fig. 10 | 21-20 | --
RH Maxi® Fuse Block | Forward of LH front Strut Tower, near Engine Compartment Fuse/Relay Center | 8A-201-7 Fig. 15 | 10-0 | --
Sensing and Diagnostic Module (SDM) | Under Driver's Seat | 8A-201-39 Fig. 75 | 202-48 | --
Starter Enable Relay | Forward of LH front Strut Tower, near Engine Compartment Fuse/Relay Center | 8A-201-7 Fig. 15 | 202-33 | --
Starter Motor | Under Intake Manifold, in Lifter Valley | 8A-201-19 Fig. 37 | -- | --
Starter Solenoid | Under Intake Manifold, on Starter Motor | 8A-201-19 Fig. 37 | -- | --
CONNECTORS:
C101 (23 Cavities) | Forward of LH front Strut Tower, near Engine Compartment Fuse/Relay Center | 8A-201-7 Fig. 15 | 202-0 | --
C131 (2 Cavities) | RH rear corner of Engine, near Cam Cover | 8A-201-23 Fig. 46 | -- | --
C202 (48 Cavities) | Below LH side of I/P, near base of Steering Column | 8A-201-29 Fig. 56 | 202-4 | --
GROUNDS:
G100 | RH front corner of Engine Compartment, on Upper Radiator Support | 8A-201-11 Fig. 22 | -- | --
G105 | RH front corner of Engine, near Generator | 8A-201-22 Fig. 47 | -- | --
SPLICES:
S103 | Body main Harness, approximately 6.5 cm for C101 connector breakout | 8A-201-7 Fig. 15 | -- | --
S121 | Engine Harness, approximately 23.5 cm from IGN1 relay connector breakout | 8A-201-7 Fig. 15 | -- | --