SMU - SECTION 3A - 5 - REVISED FRONT WHEEL ALIGNMENT SPEC.. Cadillac Concours 1996

For 1990-2009 cars

# SMU - SECTION 3A - 5 - REVISED FRONT WHEEL ALIGNMENT SPEC.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3A-5 - REVISED FRONT WHEEL ALIGNMENT SPECIFICATIONS

#### MODELS: 1995-96 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE

THIS BULLETIN REVISES THE FRONT WHEEL ALIGNMENT SPECIFICATIONS IN SECTION 3A-5 OF THE 1995 SERVICE MANUAL AND THE 1996 NPI. SPECIFICALLY, THE LEFT, RIGHT AND CROSS CAMBER SPECIFICATIONS HAVE BEEN CHANGED.

PLEASE UPDATE THE APPROPRIATE SERVICE MANUALS WITH THE NEW SPECIFICATIONS AS FOLLOWS:

SPECIFIC ITEM FROM TO ============= ==== ==

CAMBER - LEFT -0.5 DEG +/- 0.5 DEG 0.0 DEG +/- 0.5 DEG

CAMBER - RIGHT +0.5 DEG +/- 0.5 DEG 0.0 DEG +/- 0.5 DEG

CROSS CAMBER -1.0 DEG +/- 0.6 DEG 0.0 DEG +/- 0.75 DEG

ALL OTHER SPECIFICATIONS REMAIN AS ORIGINALLY PUBLISHED.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.