Low/Reverse Band and Fretting Ring Installation. Cadillac Concours 1997

For 1990-2009 cars

Note: It may be easier to install the low reverse band if it is installed on the anchor pin first.

1. Install the low reverse band (13) into the case. Be sure to properly anchor the band in the case with the servo pin stop at the case bore.
2. Install the fretting ring (835) into the case. Keep the gap in the fretting ring toward the bottom pan with the recessed area next to the anchor pin.