Engine Flywheel Removal. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

J 44214 Flywheel Holder

1. Rotate the engine so that the main bearing bolts are facing up.
2. Hold the flywheel in order to prevent rotation.
3. Loosen the 8 flywheel mounting bolts.
4. Remove 7 of the eight flywheel mounting bolts leaving one bolt at the top of the crankshaft rotation.
5. Grip the flywheel and remove the remaining bolt. Do not drop the flywheel when removing the final bolt.
6. Remove the J 44214 from the engine block.