Case Extension and Scavenge Pipe Removal. Cadillac Concours 1996

For 1990-2009 cars

1. Remove the following parts from the case extension:

• | Five 13-mm bolts (128, 129)

• | One 15-mm stud (127)

2. Remove the case extension (134) and the seal (126).
3. Remove the roller thrust bearing (132) and the selective washer (133)
4. Remove the 8-mm scavenge tube bolt (15).
5. Remove the scavenge tube (54) by prying on the differential.
6. Remove the scavenge tube seal (53).